**Electronic Code of Federal Regulations**

|  |
| --- |
| **e-CFR data is current as of May 3, 2016** |

|  |
| --- |
| [Title 29](http://www.ecfr.gov/cgi-bin/text-idx?gp=&SID=e4bb730b03c05f41301a7a88c294329b&mc=true&tpl=/ecfrbrowse/Title29/29tab_02.tpl) → [Subtitle B](http://www.ecfr.gov/cgi-bin/text-idx?gp=&SID=e4bb730b03c05f41301a7a88c294329b&mc=true&tpl=/ecfrbrowse/Title29/29subtitleB.tpl) → [Chapter XVII](http://www.ecfr.gov/cgi-bin/text-idx?gp=&SID=e4bb730b03c05f41301a7a88c294329b&mc=true&tpl=/ecfrbrowse/Title29/29chapterXVII.tpl) → [Part 1910](http://www.ecfr.gov/cgi-bin/retrieveECFR?gp=&SID=e4bb730b03c05f41301a7a88c294329b&mc=true&n=pt29.5.1910&r=PART&ty=HTML) → [Subpart D](http://www.ecfr.gov/cgi-bin/retrieveECFR?gp=&SID=e4bb730b03c05f41301a7a88c294329b&mc=true&n=sp29.5.1910.d&r=SUBPART&ty=HTML) → §1910.22 |

[Browse Previous](http://www.ecfr.gov/cgi-bin/retrieveECFR?gp=&SID=e4bb730b03c05f41301a7a88c294329b&mc=true&r=SECTION&n=se29.5.1910_121) | [Browse Next](http://www.ecfr.gov/cgi-bin/retrieveECFR?gp=&SID=e4bb730b03c05f41301a7a88c294329b&mc=true&r=SECTION&n=se29.5.1910_123)

Title 29: Labor
[PART 1910—OCCUPATIONAL SAFETY AND HEALTH STANDARDS](http://www.ecfr.gov/cgi-bin/retrieveECFR?gp=&SID=e4bb730b03c05f41301a7a88c294329b&mc=true&n=pt29.5.1910&r=PART&ty=HTML)
[Subpart D—Walking-Working Surfaces](http://www.ecfr.gov/cgi-bin/retrieveECFR?gp=&SID=e4bb730b03c05f41301a7a88c294329b&mc=true&n=sp29.5.1910.d&r=SUBPART&ty=HTML)

**§1910.22   General requirements.**

This section applies to all permanent places of employment, except where domestic, mining, or agricultural work only is performed. Measures for the control of toxic materials are considered to be outside the scope of this section.

(a) *Housekeeping.* (1) All places of employment, passageways, storerooms, and service rooms shall be kept clean and orderly and in a sanitary condition.

(2) The floor of every workroom shall be maintained in a clean and, so far as possible, a dry condition. Where wet processes are used, drainage shall be maintained, and false floors, platforms, mats, or other dry standing places should be provided where practicable.

(3) To facilitate cleaning, every floor, working place, and passageway shall be kept free from protruding nails, splinters, holes, or loose boards.

(b) *Aisles and passageways.* (1) Where mechanical handling equipment is used, sufficient safe clearances shall be allowed for aisles, at loading docks, through doorways and wherever turns or passage must be made. Aisles and passageways shall be kept clear and in good repairs, with no obstruction across or in aisles that could create a hazard.

(2) Permanent aisles and passageways shall be appropriately marked.

(c) *Covers and guardrails.* Covers and/or guardrails shall be provided to protect personnel from the hazards of open pits, tanks, vats, ditches, etc.

(d) *Floor loading protection.* (1) In every building or other structure, or part thereof, used for mercantile, business, industrial, or storage purposes, the loads approved by the building official shall be marked on plates of approved design which shall be supplied and securely affixed by the owner of the building, or his duly authorized agent, in a conspicuous place in each space to which they relate. Such plates shall not be removed or defaced but, if lost, removed, or defaced, shall be replaced by the owner or his agent.

(2) It shall be unlawful to place, or cause, or permit to be placed, on any floor or roof of a building or other structure a load greater than that for which such floor or roof is approved by the building official.