### FORM 120

Form Approved

OMB No. 0923-0048 Exp. Date 06/30/2022

**Exterior Environmental Paint Assessment**

ATSDR estimates the average public reporting burden for this collection of information as 5 minutes per response, including the time for reviewing instructions, searching existing data/information sources, gathering, and maintaining the data/information needed, and completing and reviewing the collection of information. An agency may not conduct or sponsor, and a person is not required to respond to a collection of information unless it displays a currently valid OMB Control Number. Send comments regarding this burden estimate or any other aspect of this collection of information, including suggestions for reducing this burden to CDC/ATSDR Information Collection Review Office, 1600 Clifton Road NE, MS D-74, Atlanta, Georgia 30333; ATTN: PRA (0923-0048).

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | | | \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | | |
| Place ID Sticker Here | | | Inspector and Date | | |
| **EXTERIOR** XRF Instrument No: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | | | | | | |
| Wall 1 Letter\_\_\_\_\_ Wall 2 Letter\_\_\_\_\_ Total No. Doors \_\_\_\_\_ Total No. Windows \_\_\_\_\_ | | | | | | |
| Test Component | Condition  (I or D) | Deterioration (Percent) | | XRF Result (mg/cm2) | Comments | |
| Wall 1 |  |  | |  |  | |
| Window Sash 1 |  |  | |  |  | |
| Window Trough 1 |  |  | |  |  | |
| Door 1 |  |  | |  |  | |
| Door Jamb 1 |  |  | |  |  | |
| Wall 2 |  |  | |  |  | |
| Window Sash 2 |  |  | |  |  | |
| Window Trough 2 |  |  | |  |  | |
| Door 2 |  |  | |  |  | |
| Door Jamb 2 |  |  | |  |  | |
| Main Porch |  |  | |  |  | |
| Floor |  |  | |  |  | |
| Bannister |  |  | |  |  | |
| Column |  |  | |  |  | |

Condition

* Intact (I): no obvious visible deterioration
* Fair (D): peeling, chipping, blistering, flaking, worn, chalking, alligatoring, cracking, or otherwise becoming separated from the substrate.