**ATTACHMENT D**

**Updating Labor Rates**

The Agency has updated the estimated wages, benefits and overhead for all labor categories for affected industries, state government, and EPA employees based on publicly available data from the US Bureau of Labor Statistics. The worksheets listed in this attachment describe the formulas used to estimate the labor rates and derive the fully loaded rates and overhead costs for this ICR renewal. This renewal uses **2019 base data**.

|  |  |
| --- | --- |
| Methodology | The methodology uses data on each sector and labor type for an *Unloaded wage rate* (hourly wage rate) and calculates the *Loaded wage rate* (unloaded wage rate + benefits), and the *Fully loaded wage rate* (loaded wage rate + overhead). Fully loaded wage rates are used to calculate respondent costs. This renewal uses 2019 base data. |
| Unloaded Wage Rate | Wages are estimated for labor types (management, technical, and clerical) within applicable sectors. The Agency uses average wage data for the relevant sectors available in the National Industry-Specific Occupational Employment and Wage Estimates from the Bureau of Labor Statistics (BLS) at <http://www.bls.gov/oes/current/oes_nat.htm>.  |
| Sectors | The specific North American Industry Classification System (NAICS) code and website for each sector is included in that sector’s wage rate table (see Attachment G). Within each sector, the wage data are providedby Standard Occupational Classification (SOC). The SOC system is used by Federal statistical agencies to classify workers into occupational categories for the purpose of collecting, calculating, or disseminating data (see <http://www.bls.gov/oes/current/oes_stru.htm>). |
| Loaded Wage Rate | Unless stated otherwise, all benefits represent 46% of unloaded wage rates, based on benefits for all civilian non-farm workers, from <http://www.bls.gov/news.release/ecec.t01.htm>. However, if other sectors are listed for which 46% is not applicable, the applicable percentage will be stated. |
| Fully Loaded Wage Rate | We multiply the loaded wage rate by 50% (EPA guidelines 20-70%) to get overhead costs. |

**Work Sheets to Calculate Industry and EPA Labor Costs**

**INDUSTRY LABOR COSTS**

**NAICS: 3250A1**

**Chemical Manufacturing (3251, 3252, 3253, and 3259 only)**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Labor Category: | Formula | Managerial | Technical | Clerical |
| Unloaded Hourly Rate1 | = W | $66.36 | $34.86 | $22.65 |
| Benefits Percentage2 | Lb = B/W | 46% | 46% | 46% |
| Benefits per hour | B = W\*Lb | $30.53 | $16.04 | $10.42 |
| Loaded Hourly Rate | Wb = W + B =W(1+Lb) | $96.89 | $50.90 | $33.07 |
| Overhead Percentage3 | Lo = OH/Wb | 50% | 50% | 50% |
| Overhead per hour | OH = Wb\*Lo | $48.45 | $25.45 | $16.54 |
| Fully Loaded HourlyRate | Wf = Wb + OH= W + B + OH | $145.34 | $76.35 | $49.61 |

1. Data Source: BLS <https://www.bls.gov/oes/current/naics4_3250A1.htm> **May 2019 data** NAICS 3250A1 - Chemical Manufacturing (3251, 3252, 3253, and 3259 only) Standard Occupational Codes:

Management: 11-0000, Management Occupations

Technical: 19-0000, Life, Physical, and Social Science Occupations

Clerical: 43-0000, Office and Administrative Support Occupations

2. Fringe benefits/wage per hour.

3. U. S. Environmental Protection Agency, *EPA Air Pollution Control Cost Manual, Sixth Edition*, EPA-452-02-001, January 2002, pg. 2-34. The loading for indirect costs is within the range of 20-70% of the load labor rate (wage + benefits) suggested in EPA guidance.

**EPA LABOR COSTS**

**NAICS: 999100**

**Federal Executive Branch**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Labor Category: | Formula | Managerial | Technical | Clerical |
| Unloaded Hourly Rate1 | = W | $49.52 | $36.35 | $21.05 |
| Benefits Percentage2 | Lb = B/W | 46% | 46% | 46% |
| Benefits per hour | B = W\*Lb | $22.78 | $16.72 | $9.68 |
| Loaded Hourly Rate | Wb = W + B =W(1+Lb) | $72.30 | $53.07 | $30.73 |
| Overhead Percentage3 | Lo = OH/Wb | 50% | 50% | 50% |
| Overhead per hour | OH = Wb\*Lo | $36.15 | $26.54 | $15.37 |
| Fully Loaded HourlyRate | Wf = Wb + OH= W + B + OH | $108.45 | $79.61 | $46.10 |

1. Data Source: BLS <http://www.bls.gov/oes/current/naics4_999100.htm> **May 2019 data**

NAICS 999100 - Federal Executive Branch

Standard Occupational Codes:

Management: 11-0000, Management Occupations

Technical: 19-0000, Life, Physical, and Social Science Occupations

Clerical: 43-0000, Office and Administrative Support Occupations

2. Fringe benefits/wage per hour.

3. U. S. Environmental Protection Agency, *EPA Air Pollution Control Cost Manual, Sixth Edition*, EPA-452-02-001, January 2002, pg. 2-34. The loading for indirect costs is within the range of 20-70% of the load labor rate (wage + benefits) suggested in EPA guidance.