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Posted by the Federal Motor Carrier Safety Administration on Jan 10, 2025
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Comment

It seems the dozens and dozens of primarily pickups used for transportation of personnel use rules for Warning Devices for Stopped
Commercial Motor Vehicles parked safely away from any flow of traffic yet leave bright LED "warning lights" flashing all day and all night
when NO WORKER IS NEAR. The result is a conflict with the purpose of warning lights - to warn. Drivers moving through such zones
must look all over the place to each vehicle with flashing (non) emergency warning lights attempting to determine if a person or vehicle is
actually present, who or what vehicle to pay proper attention to guaranteeing safe passage. Involved is the number of flashing
"emergency" lights, their brilliance, and whether they convey a legitimate message other than 'l can so | will'. Another favorite peeve is
tow trucks with loads secured within the flow of traffic that believe they can or must leave "emergency” lights (cough) flashing everywhere
they go. Not knowing where the need for caution is combined by blinding intensity of "emergency" lights, in my opinion causes accidents
rather than prevents them.
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