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[bookmark: _Hlk47077366]Abstract:[footnoteRef:3] [3:   The Abstract must include the following information: (1) whether responding to the collection is mandatory, voluntary, or required to obtain or retain a benefit; (2) a description of the entities who must respond; (3) whether the collection is reporting (indicate if a survey), recordkeeping, and/or disclosure; (4) the frequency of the collection (e.g., bi-annual, annual, monthly, weekly, as needed); (5) a description of the information that would be reported, maintained in records, or disclosed; (6) a description of who would receive the information; (7) the purpose of the collection; and (8) if a revision, a description of the revision and the change in burden.] 

The National Highway Traffic Safety Administration (NHTSA) is seeking approval from OMB of this information collection request (ICR) for extension with modification of its currently approved information collection for Crash Report Sampling System (CRSS). NHTSA is authorized by 49 U.S.C. § 30182 and 23 U.S.C. § 403 to collect data on motor vehicle traffic crashes to aid in the identification of issues and the development, implementation, and evaluation of motor vehicle and highway safety countermeasures. The information collected serves to identify and develop safety countermeasures that will reduce the severity of injury and property damage caused by motor vehicle crashes.  

The Crash Report Sampling System (CRSS) collects data from police-reported crashes involving all types of motor vehicles, pedestrians, and cyclists; this includes property damage only crashes as well as those resulting in injuries and fatalities.  CRSS obtains its data from a nationally representative probability sample selected from the estimated six million police-reported crashes that occur annually in the United States.  By focusing attention on police-reported crashes, CRSS concentrates on the crashes of greatest concern to the highway safety community and the general public.

CRSS depends on the voluntary participation and cooperation of State and law enforcement agencies.  This allows the National Highway Traffic Safety Administration (NHTSA) and its contractors to access the police crash reports (PCRs) to review, list, and categorize the crashes.  CRSS data is solely based on PCRs.  The PCRs provide essential data: detailed information regarding the location of the crash, the vehicles, and the people involved.  The PCRs are official local and State government forms that include the location of the crash and the pre-crash environment, explain the number and types of vehicles involved as well as describing the persons, injuries and other variables to express how the person was involved in the crash. CRSS respondents are local law enforcement agencies and State agencies that provide access to repository/website or database of motor vehicle crashes.  

For the PCR data acquisition process, NHTSA’s technicians regularly obtain PCRs from the sampled police agencies and select a sample of the in-scope PCRs. Once a PCR has been selected for data collection, NHTSA’s data coders review and retrieve the general crash information from the sampled PCR. PCR is the sole source for the CRSS data collection. 

These information collections support NHTSA’s mission to save lives and prevent injuries due to traffic crashes. The data collected from the CRSS provide annual, nationally representative estimates of the number, types, and characteristics of police-reported motor vehicle crashes. These data are used by NHTSA to support its highway safety research, policy making, and regulation program development.

[bookmark: _Hlk104906938]The previous request for this information collection (OMB No. 2127-0714) indicated 42,680 burden hours, this request decreases the burden to 18,167.  The request for the collection of information is adjusted due to a) reducing the burden hour estimates for CRSS information collection to be more accurate and reflect current efficiencies, b) removing the Non-Sampled Police Jurisdiction (PJ) Crash Count Special Study.  The removal of the Non-Sampled PJ Crash Count Special Study is the biggest change to the previous clearance. There were two special studies included in the previous clearance, Non-Sampled PJ Count Special Study and PJ Frame Evaluation Special Study. NHTSA determined the PJ Frame Evaluation Special Study is the most critical to assessing the quality of the PJ frame of the CRSS PSUs to address PJ changes and update the PJ measure of size with the latest crash counts for the CRSS PJ sample selection.  Without the PJ Frame Evaluation Special Study, NHTSA may fail to accurately assess the national crash picture by missing pertinent crash data.  Thus, if the results of the PJ Frame Evaluation Special Study reflects the current PJ landscape, the Non-Sampled PJ Crash Count Special Study is not necessary. 

The combined impact is a decrease of 24,513 burden hours to NHTSA’s overall total.  


B. COLLECTIONS OF INFORMATION EMPLOYING STATISTICAL METHODS

1. Describe the potential respondent universe and any sampling or other respondent selection methods to be used.

[bookmark: _Hlk11075153][bookmark: _Hlk11075180]CRSS is a major record-based crash data collection system.[footnoteRef:4]  CRSS is a multi-stage complex survey of police crash reports.  CRSS sample is comprised of PSU, PJ, and PCR samples.   [4:   Additional details about CRSS and how NHTSA collects this information are available in the supporting statements for the ICR with OMB Control No. 2127-0714.] 


In the following, we describe in detail the CRSS population and how the CRSS PSU, PJ, and PCR samples are selected. 

The purpose of the CRSS is to provide annual, nationally representative estimates of police-reported motor vehicle crashes as well as characteristics of these motor vehicle crashes.  PCR is the sole source of data for the CRSS.  CRSS population is the set of police-reported motor vehicle crashes on a traffic-way (strata 2 – 10 of Table 2).
[bookmark: _Toc365619289][bookmark: _Toc365626702]
Table 1.  CRSS PCR Strata, Target Sample Allocation, and Population Sizes
	CRSS
PCR Stratum
	Description
	Target Percent of Sample Allocation
	Estimated
Population 
(CRSS2023) ****
	Population Percent

	1
	An in-scope Not-in-Traffic Surveillance (NTS) crash (take all)*
	
	
	

	2
	Crashes not in Stratum 1 in which:
Involves a killed or injured (includes injury severity unknown) non-motorist
	9%
	131,072
	2.1%

	3
	Crashes not in Stratum 1 or 2 in which:
Involves a killed or injured (includes injury severity unknown) motorcycle or moped rider
	6%
	81,967
	1.3%

	4
	Crashes not in Stratum 1-3 in which:
At least one occupant of a late model year passenger vehicle** is killed or incapacitated
	4%
	20,194
	0.3%

	5
	Crashes not in Stratum 1-4 in which:
At least one occupant of an older passenger vehicle*** is killed or incapacitated
	7%
	88,363
	1.4%

	6
	Crashes not in Stratum 1-5 in which:
at least one occupant of a late model year passenger vehicle** is injured (including injury severity unknown)
	14%
	350,873
	5.7%

	7
	Crashes not in Stratum 1-6 in which:
involved at least one medium or heavy truck or bus (includes school bus, transit bus, and motor coach) with GVWR 10,000 lbs. or more
	6%
	532,028
	8.7%

	8
	Crashes not in Stratum 1-7 in which:
at least one occupant of an older passenger vehicle*** is injured (including injury severity unknown)
	12%
	862,634
	14.1%

	9.
	Crashes not in Stratum 1-8 in which:
involved at least one late model year passenger vehicle**,
AND
No person in the crash is killed or injured
	22%
	1,529,202
	24.9%

	10
	Crashes not in Stratum 1-9:
This includes mostly PDO crashes involving a non-motorist, motorcycle, moped, and passenger vehicles that are not late model year** and any crashes not classified in strata 1-9.
	20%
	2,542,026
	41.4%


*: NTS cases are not in the scope of CRSS.  They are set aside for NTS analysis.
**: Late model year passenger vehicle: passenger vehicle that are 4 years old or newer.
***: Older passenger vehicle: passenger vehicle that are 5 years old or older.
****: 2023 CRSS estimates are the most recent estimates.

The estimated CRSS population size (strata 2–10 of Table 2) was about 6.1 million in 2023.  CRSS selects a sample from the population through a stratified multi-stage cluster scheme as follows:

First Stage (PSU Sampling)
The country is divided into geographic units called Primary Sampling Units (PSUs).  A PSU is a county or group of counties and serves as a cluster.  PSUs were formed as groups of adjacent counties subject to a minimum measure of size (MOS) condition to ensure enough cases will be sampled from each PSU and weights are approximately equal within each PCR stratum defined in Table 2.  The CRSS PSU MOS was defined as:


where
       = the PCR stratum defined in Table 2. 
      = the desired total sample size of crashes 
 = the desired sample size of crashes in the PCR stratum 
 = the estimated population count of crashes in the PCR stratum 
 = the estimated population count of crashes in the PCR stratum  and PSU .

In the formula,  is the desired PCR strata sample allocation (the “Target Percent of Sample Allocation” column in Table 2), and  is the relative estimated population counts of PSU  for PCR stratum .  In this way, a PSU with a larger high interest (as defined by the oversampled PCR strata defined in Table 2) combination of estimated population counts of all PCR strata has a larger MOS.  

[bookmark: _Hlk22284429]PSU formation respects US Census region and urbanicity boundaries.  While 23 remote outlying counties in Alaska and three counties of small islands in Hawaii were excluded, the rest of the country is included in the PSU frame.  There are 707 CRSS PSUs in the PSU frame.

The PSU frame was then stratified into eight primary PSU strata by two variables – region (Northeast, West, South, and Midwest) and urbanicity (urban and rural).  Within each primary stratum, PSUs were further stratified by secondary stratification variables such as vehicle miles traveled, total crashes, truck miles traveled, and road miles by road type.  PSUs with similar characteristics were grouped into secondary strata with approximately equal MOS sizes. Secondary strata groupings were also based on minimizing the between-PSU variance within a stratum.  As the result, 50 PSU strata were formed as indicated in Table 3.

Table 2.  CRSS PSU Strata, PSU Population Counts, and Sample Size
	PRIMARY STRATA
	STRATID*
	VMT_RATE_IMP**
	TOT_CRASH
_RATE**
	TRK_MI_RATE**
	ROAD_TYPE
_RATE**
	Number of PSUs
	PSU Sample Size

	
	
	Upper
	Lower
	Upper
	Lower
	Upper
	Lower
	Upper
	Lower
	
	

	1
	101
	1801
	0
	 
	 
	 
	 
	359
	0
	5
	2

	1
	102
	4064
	1801
	 
	 
	 
	 
	359
	0
	5
	2

	1
	103
	7159
	4064
	 
	 
	 
	 
	359
	0
	8
	2

	1
	104
	5791
	0
	0.028
	0
	153756
	0
	2175
	359
	6
	2

	1
	105
	8040
	5791
	0.028
	0
	153756
	0
	2175
	359
	7
	2

	1
	106
	 
	 
	0.028
	0
	249918
	153756
	2175
	359
	7
	2

	1
	107
	 
	 
	0.028
	0
	591241
	249918
	2175
	359
	7
	2

	1
	108
	 
	 
	0.039
	0.028
	 
	 
	2175
	359
	11
	2

	2
	201
	 
	 
	 
	 
	236701
	0
	 
	 
	22
	2

	2
	202
	 
	 
	 
	 
	1027526
	236701
	 
	 
	22
	2

	3
	301
	4135
	0
	 
	 
	45709
	0
	 
	 
	3
	2

	3
	302
	7465
	4135
	 
	 
	45709
	0
	 
	 
	8
	2

	3
	303
	9898
	7465
	 
	 
	45709
	0
	 
	 
	10
	2

	3
	304
	 
	 
	 
	 
	102554
	45709
	 
	 
	11
	2

	3
	305
	4444
	0
	 
	 
	339758
	102554
	 
	 
	13
	2

	3
	306
	6003
	4444
	 
	 
	339758
	102554
	 
	 
	11
	2

	3
	307
	11618
	6003
	 
	 
	339758
	102554
	 
	 
	10
	2

	4
	401
	 
	 
	 
	 
	66171
	0
	4345
	0
	28
	2

	4
	402
	6045
	0
	 
	 
	565025
	66171
	4345
	0
	27
	2

	4
	403
	11623
	6045
	 
	 
	565025
	66171
	4345
	0
	25
	2

	4
	404
	 
	 
	 
	 
	 
	 
	17641
	4345
	30
	2

	5
	501
	3620
	0
	0.048
	0
	125590
	0
	 
	 
	5
	2

	5
	502
	4530
	3620
	0.048
	0
	125590
	0
	 
	 
	8
	2

	5
	03
	4951
	4530
	0.048
	0
	125590
	0
	 
	 
	6
	2

	5
	504
	5016
	4951
	0.048
	0
	125590
	0
	 
	 
	3
	2

	5
	505
	5277
	5016
	0.048
	0
	125590
	0
	 
	 
	5
	2

	5
	506
	5746
	5277
	0.048
	0
	125590
	0
	 
	 
	6
	2

	5
	507
	6399
	5746
	0.048
	0
	125590
	0
	 
	 
	5
	2

	5
	508
	12826
	6399
	0.048
	0
	125590
	0
	 
	 
	8
	2

	5
	509
	5641
	0
	0.048
	0
	210430
	125590
	 
	 
	6
	2

	5
	510
	8348
	5641
	0.048
	0
	210430
	125590
	 
	 
	7
	2

	5
	511
	13892
	8348
	0.048
	0
	210430
	125590
	 
	 
	10
	2

	5
	512
	 
	 
	0.048
	0
	358684
	210430
	 
	 
	8
	2

	5
	513
	 
	 
	0.048
	0
	877546
	358684
	 
	 
	13
	2

	5
	514
	 
	 
	0.085
	0.048
	 
	 
	 
	 
	17
	2

	6
	601
	 
	 
	 
	 
	49854
	0
	 
	 
	35
	2

	6
	602
	6353
	0
	 
	 
	162415
	49854
	 
	 
	34
	2

	6
	603
	14415
	6353
	 
	 
	162415
	49854
	 
	 
	35
	2

	6
	604
	 
	 
	 
	 
	250190
	162415
	 
	 
	33
	2

	6
	605
	5693
	0
	 
	 
	1156242
	250190
	 
	 
	35
	2

	6
	606
	16271
	5693
	 
	 
	1156242
	250190
	 
	 
	35
	2

	7
	700
	 
	 
	 
	 
	 
	 
	 
	 
	1
	1

	7
	701
	6477
	0
	0.027
	0
	104522
	0
	 
	 
	7
	2

	7
	702
	6921
	6477
	0.027
	0
	104522
	0
	 
	 
	4
	2

	7
	703
	7861
	6921
	0.027
	0
	104522
	0
	 
	 
	5
	2

	7
	704
	5137
	0
	0.027
	0
	249358
	104522
	 
	 
	3
	2

	7
	705
	8070
	5137
	0.027
	0
	249358
	104522
	 
	 
	10
	2

	7
	706
	 
	 
	0.048
	0.027
	92716
	0
	 
	 
	9
	2

	7
	707
	 
	 
	0.048
	0.027
	186409
	92716
	 
	 
	7
	2

	8
	801
	 
	 
	 
	 
	 
	 
	3938
	0
	30
	2

	8
	802
	 
	 
	 
	 
	 
	 
	18292
	3938
	41
	2


*: STRATID: Secondary PSU ID. 
**: VMT_RATE_IMP = imputed vehicle miles traveled / (PSU MOS×1,000,000). 
      TOT_CRASH_RATE = (imputed 2008 injury crashes + imputed 2008 PDO crashes + 2007-2011 average fatal 
      crashes) / (PSU MOS×1,000,000). 
     TRK_MI_RATE = Total truck miles / (PSU MOS×1,000,000). 
     ROAD_TYPE_RATE = (primary road miles + secondary road miles) / (PSU MOS×1,000,000). 
A major challenge of the CRSS sample design is the uncertainty of the future operational budget.  Due to unknown future funding levels and the need for a stable PSU sample, NHTSA implemented a scalable PSU sample, which allows for the PSU sample size to be decreased or increased with minimum impact to the existing PSU sample and for the selection probabilities to be tracked.  To this end, a multi-phase sampling method was used to select the CRSS PSU sample by selecting a sequence of nested PSU samples.  In this method, a PSU sample larger than what is actually needed is selected during the first phase of the PSU sample.  From the first phase of the PSU sample, a smaller subset of the PSU sample is selected as the second phase of the PSU sample.  From the second phase of the PSU sample, another smaller third phase of the PSU sample is selected.  This process is continued until the PSU sample size reaches unacceptable levels.  In this way, a sequence of nested PSU samples is obtained.  Each of these PSU samples is a probability sample and can be used for data collection (see Figure 2).  According to the prevailing budget level, a sample with the appropriate sample size is picked from the nested sequence.  This allows us to easily track the selection probabilities and minimizes changes to the existing PSU sample.

Figure 1.  Nested PSU Samples for CRSS

For the CRSS, five PSU samples were selected under the five scenarios.  Table 4 summarizes the number of PSU strata and sampled PSUs for the CRSS PSU sample scenarios. 

Table 3.  CRSS PSU Sample Scenarios: Number of Strata and Sample Size
	Scenario
	Number of PSU Strata
	Number of Sampled Non-certainty PSUs
	Number of Sampled Certainty PSUs
	Total Number of Sampled PSUs

	1
	50
	97
	4
	101

	2
	37
	74
	1
	75

	3
	25
	50
	1
	51

	4
	12
	24
	0
	24

	5
	8
	16
	0
	16



For scenario 1, with a sample size of 100 and without stratification, one PSU was identified as a certainty PSU by the condition:



Here N is the total number of PSUs in the PSU frame and i is an index for a PSU.  The PSU selected with certainty[footnoteRef:5] was set aside.  Then two PSUs were selected using proportional to size (PPS) sampling from each of the 50 scenario-1 strata.  With the sample size of two for each PSU stratum, three PSUs were identified as certainty PSUs by the condition:  [5:  In the probability proportional to size (PPS) sampling, a certainty PSU is identified when the selection probability is calculated to be greater than or equal to one.  If a PSU is identified as certainty, it must be in the sample and its selection probability is set to one.  A non-certainty PSU is selected with its selection probability that is greater than 0 and less than 1.  If a PSU has a selection probability closer to one, it has more chance to be in the sample.  On the other hand, if a PSU has a selection probability closer to zero, it has less chance to be in the sample.  For more details, please see Pages 13-28 in the published Technical Report https://crashstats.nhtsa.dot.gov/Api/Public/ViewPublication/812706
] 




Here  is the total number of PSUs in stratum .  The certainty PSUs selected with certainty were set aside.  The corresponding stratum PSU sample size was reduced by one.  Then a PPS sample of non-certainty PSUs was selected using the reduced PSU stratum sample size.

Scenario-1 sample has 101 PSUs.  For a non-certainty PSU, the selection probability is:



Here  be the non-certainty PSU sample size for PSU stratum .

For scenario-2, with a sample size of 74 and without stratification, one PSU was identified as a certainty PSU and was set aside.  Then 13 of the scenario-1 strata were collapsed with other strata to form the 37 scenario-2 PSU strata.  The collapsing of strata follows the following rules: 

· Only the secondary strata in the same primary stratum can be collapsed;
· Only the contiguous secondary strata can be collapsed; 
· The resulting strata has a similar stratum total MOS within each primary stratum.  

In each of the scenario-2 stratum, the sampled scenario-1 PSUs were treated as the sampling frame.  Each PSU was assigned a new MOS equal to its scenario-1 stratum total MOS.  Then two PSUs were selected from each scenario-2 stratum using PPS sampling based on the new MOS.  In this way, the resulting selection probability of the scenario-2 PSU is still PPS selection probability. Other scenario samples were selected in a similar way.

The current CRSS PSU sample size is 61 (between scenarios 2 and 3) with 60 responding PSUs and one non-responding PSU. 

Second Stage (PJ Sampling)
The secondary sampling units (SSU) of CRSS are police jurisdictions (PJs) that produce PCRs for the crashes occurred within the sampled PSUs.  A composite MOS is assigned to each PJ in the selected PSUs.  Similar to the PSU MOS definition, it is sensible to assign larger selection probabilities to PJs with more high interest crashes as defined by the oversampled strata in Table 2.  For each PJ in the selected PSUs, crash counts from the 9 PCR strata in Table 2 (Stratum 2-10) were estimated from the information collected from the PJs in the selected PSUs.  For PJ  in the PJ frame within the sampled PSU , the composite SSU MOS is defined as the following:


where
       = the PCR stratum defined in Table 2. 
      = the desired total sample size of crashes
  = the desired sample size of crashes in the PCR stratum 
 = the estimated population count of crashes in PCR stratum 
 = the estimated population count of crashes in PCR stratum , PJ  and PSU 

PJs are then stratified into two PJ strata by their MOS (large MOS stratum [largest 50%] and small MOS stratum [the rest]) in addition to certainty PJ stratum where all PJs are selected with certainty.  A PJ sample is selected using Pareto sampling.  The Pareto sampling method produces an approximate PPS sample, handles the frame changes and minimizes the changes to the existing sample at the same time.  Pareto sampling method was applied to the PJ sample selection for each of the non-certainty PJ strata (large MOS and small MOS stratum) within the sampled PSU, as the following: 

Step 1: Generate a permanent uniform random number  for each PJ  in the PJ stratum h of PSU i.  
Step 2: Identify certainty PJs by the condition: 



Here  is the PJ sample size and  is the PJ frame size for PJ stratum h within PSU i.   is the PJ MOS.  
Step 3: The identified certainty PJs are set aside.  This process is repeated for the remaining PJs based on the reduced PJ sample size until there are no more certainty PJs.  Let the total number of certainty PJs be . For the remaining  non-certainty PJs in the frame, calculate the PPS inclusion probability with the non-certainty PJ sample size (



Step 4: Calculate the transformed random numbers and sort the transformed random numbers from the smallest to the largest as following: 



Step 5: The  certainty PJs plus the first  non-certainty PJs from the above list are the PJ sample for PJ stratum h within PSU .  

Pareto sampling is approximately PPS, and the PJ selection probability is:



The 2023 CRSS PJ sample size is 289. 

Third Stage (PCR Sampling)
The tertiary sampling units (TSU) of CRSS are PCRs.  The CRSS PCR sample is selected by stratified systematic sampling.  For each selected SSU (PJ), PCRs are periodically obtained by either a technician’s visit to the PJ or electronic transmission.  All the PCRs are listed in the order they become available and are stratified by the PCR strata identified in Table 2.  Through this listing process, the PCR sampling frame in each selected PJ is prepared for PCR sample selection.  

For a large PJ with too many PCRs to be listed, PCRs are sub-listed by systematic sampling.  For example, only PCRs with a PCR number ending in 0 through 4 may be listed if the sub-listing factor is 2 (i.e., 5 PCRs among 10 PCRs are listed).  Or only PCRs with a PCR number ending in 0 or 1 are listed if the sub-listing factor is 5 (i.e., 2 PCRs among 10 PCRs are listed).  If  PCRs among 10 PCRs are sub-listed in PJ  in PSU , the sub-listing probability for all sub-listed PCRs are:



[bookmark: _Hlk81294732]After PCRs are listed, a PCR sample is selected by systematic sampling from the listed (or sub-listed) PCRs by PCR stratum within each selected PJ.  The selection probability of PCR   from PCR stratum  is:



Here   is the PSU selection probability,  is the PJ selection probability, and  is the sub-listing probability.  , which is the sampling rate of the PCR stratum , is calculates with the target PCR sample size  and the estimated total number of PCRs in the population for the PCRs stratum  as: 



The overall selection probability is: 



The design weight is the inverse of .  

Sample Allocation
For a three-stage sample design as this program, the PSU, SSU and TSU sample sizes can be estimated using optimization by minimizing the variance subject to cost assuming a three-stage simple random sampling without replacement.  

The optimization model consists of the objective function, cost constraint, and variance constrains as the following:      
                       




where
: Subscript of the identified key variable, .  
:  Proportion estimate of the key variable. 
: Optimal sample sizes of PSUs, SSUs per PSU, and TSUs per SSU to be determined.  
: Population size of PSUs 
: Average population size of SSUs.    
: Average population size of TSUs. 
: Variance of the identified key estimate . 
: Variance component at PSU-, SSU-, and TSU-level. 
: Total, fixed, PSU-, SSU-, and TSU-level cost coefficients.  
: Variance of the identified key estimate  in General Estimates System (GES)[footnoteRef:6].  [6:  https://www.nhtsa.gov/national-automotive-sampling-system/nass-general-estimates-system] 


Figure 3 displays the optimization results.  As the rescaled budget increases, the PJ sample size m and the PCR sample size k tend to be stable while the PSU sample size n increases and the average variance decreases.  Since there are 9 PCR domains to be estimated (strata 2-10 in Table 1), the final PCR sample size is 9×k. 

Figure 2: Average Variance, PSU, PJ and PCR Sample Size as Functions of Budget

Note: All costs are rescaled, so the lowest cost starts from $1.
Each year, CRSS’s target sample is 50,000 crashes.  Below is a table summarizing the CRSS sample.  The 2016 CRSS data collection year had only 53 PSUs instead of the full 60 PSUs due to constraints with receiving police crash reports, thus the sample was less than the anticipated 50,000 crashes. 

Table 4: Unweighted Summary Statistics
	Year
	Crashes
	Vehicles 
	People
	Drivers
	Occupants
	Pedestrians
	Pedalcyclists

	
	
	(In-Transport)
	
	
	
	
	

	2016
	46,511
	82,149
	117,759
	82,000
	113,405
	2,257
	1,576

	2017
	54,969
	97,625
	138,913
	97,388
	133,408
	2,881
	1,946

	2018
	48,443
	86,105
	120,230
	85,916
	115,774
	2,444
	1,436

	2019
	54,409
	96,717
	135,410
	96,488
	129,980
	2,949
	1,802

	2020
	54,745
	94,718
	131,962
	94,500
	126,460
	2,882
	1,923

	2021
	54,200
	95,785
	133,734
	95,551
	128,315
	2,886
	1,820

	2022
	53,955
	94,756
	132,175
	94,510
	126,442
	2,967
	1,870

	2023
	50,103
	87,461
	122,388
	87,262
	116,597
	2,907
	2,050



More information on CRSS Sample Design and Weighting can be found at https://crashstats.nhtsa.dot.gov/Api/Public/ViewPublication/812706

Describe collection of information procedures.

CRSS data collection efforts are dependent on the method in which the crash reports are accessed.  The crash reports are accessed through NHTSA’s Electronic Data Transfer (EDT) program, data feeds, secure email, State websites, or manually by contract staff that physically visit the police jurisdiction.

The EDT program consists of a routine automated transfer of crash data from the State crash database to NHTSA.  EDT reduces the level of effort required to share crash data because data is automatically shared nightly from the State to NHTSA.  States may also provide crash reports to NHTSA through secure web service portals on a routine basis.  The State designates the frequency with which they share data with NHTSA under this protocol.  Crash report accessed via EDT and secure web portal are uploaded into the Police Accident Report Sampling Engine (PARSE).  The PARSE application is a centralized, web-based repository in which CRSS applicable crash reports are listed, categorized, and selected for further coding. In 2023, over one third (21 out of 60) of CRSS PSUs are EDT PSUs.  

Alternatively, States may provide access to their crash data collection websites.  States provide log-in credentials to view crash reports for the sample PJs.  The sampler would then list, categorize, and sample the crash reports for sample agencies within the PARSE application.

When States are not able to provide electronic access to crash reports, NHTSA seeks manual access to crash reports from individual police jurisdictions identified in the CRSS sample.  Generally, this includes visiting the office to access paper or electronic files, uploading crash reports on an encrypted thumb drive, linking crash reports to a secure email or copying crash reports and sending the crash reports via mail courier service.  These manual processes are completed on a schedule established by the police agency.  Once the schedule is agreed upon, then the CRSS sampler can view, list, categorize, and sample the crash reports within the PARSE application. In 2023 CRSS, for example, NHTSA obtained cooperation from 254 PJs in 39 non-EDT PSUs.

Describe methods to maximize response rates and to deal with issues of non-response.

CRSS has a three-stage sample design.  The first stage sampling units or PSUs are counties or groups of counties.  A PSU becomes a non-responding PSU only if all selected police jurisdictions (PJs) within the PSU are non-responding PJs.  Since the PJ sample is selected using the Pareto sampling method, all PJs in the PJ frame can be selected as replacement sample for non-responding PJs.  Therefore, a PSU becomes a non-responding PSU only if all PJs in the frame are non-responding PJs.  In 2017 CRSS, one PSU was non-responding.  Since the CRSS PSU sample is scalable, we increased the sample size from 60 to 61 and selected a replacement PSU without changing the original PSU sample. The weight of the non-responding PSU was adjusted. 

The second stage sampling units of CRSS are PJs.  A sampled PJ becomes non-responding PJ if it refuses to cooperate.  To improve PJ cooperation rate, NHTSA visits each selected PJ and meets with local law enforcement officers to gain cooperation.  In 2023 CRSS, 14 PJs among the 268 sampled PJs in non-EDT PSUs were non-responding.  The weights of non-responding PJs were adjusted. 

The third stage sampling units of CRSS are PCRs.  First all police crash reports (PCRs) in the selected PJs are listed.  Then a systematic sample of PCRs is selected and coded.  A PCR is identified as non-responding if it has un-readable pages or missing pages.  In 2023 CRSS for example, only 21 PCRs among the 50,241 sampled PCRs were non-responding.  The weights of the non-responding PCRs were adjusted.

The CRSS quality control system is designed to produce the most accurate, reliable, and complete database possible within the limits of available resources.  Each selected case is reviewed by quality control personnel for accuracy before proceeding to coding.  Additionally, PARSE automatically selects five percent from each sample of non-selected cases to review.  The findings from the listed cases review helps identify any quality control issues and additional training needs for the CRSS Sampler.



4. Describe any tests of procedures or methods to be undertaken.

There is no tests procedure to be undertaken at this time.

Provide the name and telephone number of individuals consulted on statistical aspects of the design and the name of the agency unit, contractor(s), grantee(s), or other person(s) who will actually collect and/or analyze the information for the agency.

Ms. Chou-Lin Chen, National Center for Statistics and Analysis, NHTSA, is responsible for CISS survey design and special studies.

NHTSA contracted with Westat (contract DTNH22-12-F-00389) on the CRSS survey design effort.  NHTSA has contracted with Westat (contract GS00Q14OADU223/ task order 693JJ924F000013) to provide statistical support on the CRSS. 

NHTSA has contracted with Laansu Inc. (contract 693JJ921C000009 and 693JJ922C000011) for the data collection, coding and quality control for the CRSS data collection effort.


Scenario 1: 101 PSUs


Scenario 2: 75 PSUs 


Scenario 3: 51 PSUs


Scenario 4: 24 PSUs


Scenario 5: 16 PSUs


Average Variance, n, m, and k as Functions of Budget
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