For FERC-717 (18CFR 37.5, 37.8, and 38):

PART 37—OPEN ACCESS SAME-TIME INFORMATION SYSTEMS

….

§ 37.5 Obligations of Transmission Providers and Responsible Parties.

(a) Each Transmission Provider is required to provide for the operation of an OASIS, either individually or jointly with other Transmission Providers, in accordance with the requirements of this Part. The Transmission Provider may delegate this responsibility to a Responsible Party such as another Transmission Provider, an Independent System Operator, a Regional Transmission Group, or a Regional Reliability Council.

(b) A Responsible Party must provide access to an OASIS providing standardized information relevant to the availability of transmission capacity, prices, and other information (as described in this part) pertaining to the transmission system for which it is responsible.

(c) A Responsible Party may not deny or restrict access to an OASIS user merely because that user makes automated computer-to-computer file transfers or queries, or extensive requests for data.

(d) In the event that an OASIS user's grossly inefficient method of accessing an OASIS node or obtaining information from the node seriously degrades the performance of the node, a Responsible Party may limit a user's access to the OASIS node without prior Commission approval. The Responsible Party must immediately contact the OASIS user to resolve the problem. Notification of the restriction must be made to the Commission within two business days of the incident and include a description of the problem. A closure report describing how the problem was resolved must be filed with the Commission within one week of the incident.

(e) In the event that an OASIS user makes an error in a query, the Responsible Party can block the affected query and notify the user of the nature of the error. The OASIS user must correct the error before making any additional queries. If there is a dispute over whether an error has occurred, the procedures in paragraph (d) of this section apply.

(f) Transmission Providers must provide “read only” access to the OASIS to Commission staff and the staffs of State regulatory authorities, at no cost, after such staff members have complied with the requisite registration procedures.

**§ 37.8 Obligations of OASIS users.**

Each OASIS user must notify the Responsible Party one month in advance of initiating a significant amount of automated queries. The OASIS user must also notify the Responsible Party one month in advance of expected significant increases in the volume of automated queries.

**PART 38—BUSINESS PRACTICE STANDARDS AND COMMUNICATION PROTOCOLS FOR PUBLIC UTILITIES**

**§ 38.1 Applicability.**

This part applies to any public utility that owns, operates, or controls facilities used for the transmission of electric energy in interstate commerce or for the sale of electric energy at wholesale in interstate commerce and to any non-public utility that seeks voluntary compliance with jurisdictional transmission tariff reciprocity conditions.

**§ 38.2 Incorporation by reference of North American Energy Standards Board Wholesale Electric Quadrant standards.**

(a) All entities to which § 38.1 is applicable must comply with the following business practice and electronic communication standards promulgated by the North American Energy Standards Board Wholesale Electric Quadrant, which are incorporated herein by reference:

(1) Open Access Same-Time Information Systems (OASIS), Version 1.5 (WEQ-001, Version 002.1, March 11, 2009, with minor corrections applied May 29, 2009 and September 8, 2009, with the exception of Standards 001-0.1, 001-0.9 through 001-0.13, 001-1.0, 001-9.7, 001-14.1.3, and 001-15.1.2);

(2) Open Access Same-Time Information Systems (OASIS) Standards & Communication Protocols, Version 1.5 (WEQ-002, Version 002.1, March 11, 2009, with minor corrections applied May 29, 2009 and September 8, 2009);

(3) Open Access Same-Time Information Systems (OASIS) Data Dictionary, Version 1.5 (WEQ-003, Version 002.1, March 11, 2009, with minor corrections applied May 29, 2009 and September 8, 2009);

(4) Coordinate Interchange (WEQ-004, Version 002.1, March 11, 2009, with minor corrections applied May 29, 2009 and September 8, 2009);

(5) Area Control Error (ACE) Equation Special Cases (WEQ-005, Version 002.1, March 11, 2009, with minor corrections applied May 29, 2009 and September 8, 2009);

(6) Manual Time Error Correction (WEQ-006, Version 001, Oct. 31, 2007, with minor corrections applied on Nov. 16, 2007);

(7) Inadvertent Interchange Payback (WEQ-007, Version 002.1, March 11, 2009, with minor corrections applied May 29, 2009 and September 8, 2009);

(8) Transmission Loading Relief—Eastern Interconnection (WEQ-008, Version 002.1, March 11, 2009, with minor corrections applied May 29, 2009 and September 8, 2009);

(9) Gas/Electric Coordination (WEQ-011, Version 002.1, March 11, 2009, with minor corrections applied May 29, 2009 and September 8, 2009);

(10) Public Key Infrastructure (PKI) (WEQ-012, Version 002.1, March 11, 2009, with minor corrections applied on May 29, 2009 and September 8, 2009);

(11) Open Access Same-Time Information Systems (OASIS) Implementation Guide, Version 1.5 (WEQ-013, Version 002.1, March 11, 2009, with minor corrections applied on May 29, 2009 and September 8, 2009); and

(12) Business Practices for Measurement and Verification of Wholesale Electricity Demand Response (WEQ-015, 2010 Annual Plan Items 4(a) and 4(b), March 21, 2011).

(13) Business Practice Standards for Measurement and Verification of Energy Efficiency Products (WEQ-021, 2010 Annual Plan Item 4(d), May 13, 2011).

(b) This incorporation by reference was approved by the Director of the Federal Register in accordance with 5 U.S.C. 552(a) and 1 CFR part 51. Copies of these standards may be obtained from the North American Energy Standards Board, 801 Travis Street, Suite 1675, Houston, TX 77002, Tel: (713) 356-0060. NAESB's Web site is at *http://www.naesb.org/.* Copies may be inspected at the Federal Energy Regulatory Commission, Public Reference and Files Maintenance Branch, 888 First Street, NE., Washington, DC 20426, Tel: (202) 502-8371, *http://www.ferc.gov,* or at the National Archives and Records Administration (NARA). For information on the availability of this material at NARA, call 202-741-6030, or go to: [*http://www.archives.gov/federal\_register/code\_of\_federal\_regulations/ibr\_locations.html*](http://www.archives.gov/federal_register/code_of_federal_regulations/ibr_locations.html)*.*

**For FERC-917 (18CFR 35.28(c), (d), and (e)):**

[PART 35—FILING OF RATE SCHEDULES AND TARIFFS](http://www.ecfr.gov/cgi-bin/retrieveECFR?gp=&SID=32cddb825de9f1fbe294e63e5db959c2&n=18y1.0.1.2.23&r=PART&ty=HTML)  
[Subpart C—Other Filing Requirements](http://www.ecfr.gov/cgi-bin/retrieveECFR?gp=&SID=32cddb825de9f1fbe294e63e5db959c2&n=18y1.0.1.2.23.3&r=SUBPART&ty=HTML)

**§ 35.28 Non-discriminatory open access transmission tariff.**

….

(c) *Non-discriminatory open access transmission tariffs.*

(1) Every public utility that owns, controls, or operates facilities used for the transmission of electric energy in interstate commerce must have on file with the Commission an open access transmission tariff of general applicability for transmission services, including ancillary services, over such facilities. Such tariff must be the *pro forma* tariff promulgated by the Commission, as amended from time to time, or such other tariff as may be approved by the Commission consistent with the principles set forth in Commission rulemaking proceedings promulgating and amending the *pro forma* tariff.

(i) Subject to the exceptions in paragraphs (c)(1)(ii), (c)(1)(iii), (c)(1)(iv), and (c)(1)(v) of this section, the open access transmission tariff, which tariff must be the *pro forma* tariff required by Commission rulemaking proceedings promulgating and amending the *pro forma* tariff, and accompanying rates must be filed no later than 60 days prior to the date on which a public utility would engage in a sale of electric energy at wholesale in interstate commerce or in the transmission of electric energy in interstate commerce.

(ii) If a public utility owns, controls, or operates facilities used for the transmission of electric energy in interstate commerce, it must file the revisions to its open access transmission tariff required by Commission rulemaking proceedings promulgating and amending the *pro forma* tariff, pursuant to section 206 of the FPA and accompanying rates pursuant to section 205 of the FPA in accordance with the procedures set forth in Commission rulemaking proceedings promulgating and amending the *pro forma* tariff.

(iii) If a public utility owns, controls, or operates transmission facilities used for the transmission of electric energy in interstate commerce, such facilities are jointly owned with a non-public utility, and the joint ownership contract prohibits transmission service over the facilities to third parties, the public utility with respect to access over the public utility's share of the jointly owned facilities must file the revisions to its open access transmission tariff required by Commission rulemaking proceedings promulgating and amending the *pro forma* tariff pursuant to section 206 of the FPA and accompanying rates pursuant to section 205 of the FPA in accordance with the procedures set forth in Commission rulemaking proceedings promulgating and amending the *pro forma* tariff.

(iv) Any public utility whose transmission facilities are under the independent control of a Commission-approved ISO or RTO may satisfy its obligation under paragraph (c)(1) of this section, with respect to such facilities, through the open access transmission tariff filed by the ISO or RTO.

(v) If a public utility obtains a waiver of the tariff requirement pursuant to paragraph (d) of this section, it does not need to file the open access transmission tariff required by this section.

(vi) Any public utility that seeks a deviation from the *pro forma* tariff promulgated by the Commission, as amended from time to time, must demonstrate that the deviation is consistent with the principles set forth in Commission rulemaking proceedings promulgating and amending the *pro forma* tariff.

(vii) Each public utility's open access transmission tariff must include the standards incorporated by reference in part 38 of this chapter.

(2) Subject to the exceptions in paragraphs (c)(2)(i) and (c)(3)(iii) of this section, every public utility that owns, controls, or operates facilities used for the transmission of electric energy in interstate commerce, and that uses those facilities to engage in wholesale sales and/or purchases of electric energy, or unbundled retail sales of electric energy, must take transmission service for such sales and/or purchases under the open access transmission tariff filed pursuant to this section.

(i) For sales of electric energy pursuant to a requirements service agreement executed on or before July 9, 1996, this requirement will not apply unless separately ordered by the Commission. For sales of electric energy pursuant to a bilateral economy energy coordination agreement executed on or before July 9, 1996, this requirement is effective on December 31, 1996. For sales of electric energy pursuant to a bilateral non-economy energy coordination agreement executed on or before July 9, 1996, this requirement will not apply unless separately ordered by the Commission.

(ii) [Reserved]

(3) Every public utility that owns, controls, or operates facilities used for the transmission of electric energy in interstate commerce, and that is a member of a power pool, public utility holding company, or other multi-lateral trading arrangement or agreement that contains transmission rates, terms or conditions, must have on file a joint pool-wide or system-wide open access transmission tariff, which tariff must be the *pro forma* tariff promulgated by the Commission, as amended from time to time, or such other open access transmission tariff as may be approved by the Commission consistent with the principles set forth in Commission rulemaking proceedings promulgating and amending the *pro forma* tariff.

(i) For any power pool, public utility holding company or other multi-lateral arrangement or agreement that contains transmission rates, terms or conditions and that is executed after October 11, 2011, this requirement is effective on the date that transactions begin under the arrangement or agreement.

(ii) For any power pool, public utility holding company or other multi-lateral arrangement or agreement that contains transmission rates, terms or conditions and that is executed on or before May 14, 2007, a public utility member of such power pool, public utility holding company or other multi-lateral arrangement or agreement that owns, controls, or operates facilities used for the transmission of electric energy in interstate commerce must file the revisions to its joint pool-wide or system-wide open access transmission tariff required by Commission rulemaking proceedings promulgating and amending the *pro forma* tariff pursuant to section 206 of the FPA and accompanying rates pursuant to section 205 of the FPA in accordance with the procedures set forth in Commission rulemaking proceedings promulgating and amending the *pro forma* tariff.

(iii) A public utility member of a power pool, public utility holding company or other multi-lateral arrangement or agreement that contains transmission rates, terms or conditions and that is executed on or before July 9, 1996 must take transmission service under a joint pool-wide or system-wide open access transmission tariff filed pursuant to this section for wholesale trades among the pool or system members.

(4) Consistent with paragraph (c)(1) of this section, every Commission-approved ISO or RTO must have on file with the Commission an open access transmission tariff of general applicability for transmission services, including ancillary services, over such facilities. Such tariff must be the *pro forma* tariff promulgated by the Commission, as amended from time to time, or such other tariff as may be approved by the Commission consistent with the principles set forth in Commission rulemaking proceedings promulgating and amending the *pro forma* tariff.

(i) Subject to paragraph (c)(4)(ii) of this section, a Commission-approved ISO or RTO must file the revisions to its open access transmission tariff required by Commission rulemaking proceedings promulgating and amending the *pro forma* tariff pursuant to section 206 of the FPA and accompanying rates pursuant to section 205 of the FPA in accordance with the procedures set forth in Commission rulemaking proceedings promulgating and amending the *pro forma* tariff.

(ii) If a Commission-approved ISO or RTO can demonstrate that its existing open access transmission tariff is consistent with or superior to the *pro forma* tariff promulgated by the Commission, as amended from time to time, the Commission-approved ISO or RTO may instead set forth such demonstration in its filing pursuant to section 206 in accordance with the procedures set forth in Commission rulemaking proceedings promulgating and amending the *pro forma* tariff.

(d) *Waivers.* A public utility subject to the requirements of this section and Order No. 889, FERC Stats. & Regs. ¶ 31,037 (Final Rule on Open Access Same-Time Information System and Standards of Conduct) may file a request for waiver of all or part of the requirements of this section, or Part 37 (Open Access Same-Time Information System and Standards of Conduct for Public Utilities), for good cause shown. Except as provided in paragraph (f) of this section, an application for waiver must be filed no later than 60 days prior to the time the public utility would have to comply with the requirement.

(e) *Non-public utility procedures for tariff reciprocity compliance.* (1) A non-public utility may submit an open access transmission tariff and a request for declaratory order that its voluntary transmission tariff meets the requirements of Commission rulemaking proceedings promulgating and amending the *pro forma* tariff.

(i) Any submittal and request for declaratory order submitted by a non-public utility will be provided an NJ (non-jurisdictional) docket designation.

(ii) If the submittal is found to be an acceptable open access transmission tariff, an applicant in a Federal Power Act (FPA) section 211 or 211A proceeding against the non-public utility shall have the burden of proof to show why service under the open access transmission tariff is not sufficient and why a section 211 or 211A order should be granted.

(2) A non-public utility may file a request for waiver of all or part of the reciprocity conditions contained in a public utility open access transmission tariff, for good cause shown. An application for waiver may be filed at any time.

**For FERC-918 (18CFR 37.6 and 37.7):**

**PART 37—OPEN ACCESS SAME-TIME INFORMATION SYSTEMS**

**§ 37.6 Information to be posted on the OASIS.**

(a) The information posted on the OASIS must be in such detail and the OASIS must have such capabilities as to allow Transmission Customers to:

(1) Make requests for transmission services offered by Transmission Providers, Resellers and other providers of ancillary services, request the designation of a network resource, and request the termination of the designation of a network resource;

(2) View and download in standard formats, using standard protocols, information regarding the transmission system necessary to enable prudent business decision making;

(3) Post, view, upload and download information regarding available products and desired services;

(4) Clearly identify the degree to which transmission service requests or schedules were denied or interrupted;

(5) Obtain access, in electronic format, to information to support available transmission capability calculations and historical transmission service requests and schedules for various audit purposes; and

(6) Make file transfers and automated computer-to-computer file transfers and queries as defined by the Standards and Communications Protocols Document.

(b) *Posting transfer capability.* The available transfer capability on the Transmission Provider's system (ATC) and the total transfer capability (TTC) of that system shall be calculated and posted for each Posted Path as set out in this section.

(1) *Definitions.* For purposes of this section the terms listed below have the following meanings:

(i) *Posted path* means any control area to control area interconnection; any path for which service is denied, curtailed or interrupted for more than 24 hours in the past 12 months; and any path for which a customer requests to have ATC or TTC posted. For this last category, the posting must continue for 180 days and thereafter until 180 days have elapsed from the most recent request for service over the requested path. For purposes of this definition, an hour includes any part of an hour during which service was denied, curtailed or interrupted.

(ii) *Constrained posted path* means any posted path having an ATC less than or equal to 25 percent of TTC at any time during the preceding 168 hours or for which ATC has been calculated to be less than or equal to 25 percent of TTC for any period during the current hour or the next 168 hours.

(iii) *Unconstrained posted path* means any posted path not determined to be a constrained posted path.

(iv) The word *interconnection,* as used in the definition of “posted path”, means all facilities connecting two adjacent systems or control areas.

(v) *Available transfer capability* or *ATC* means the transfer capability remaining in the physical transmission network for further commercial activity over and above already committed uses, or such definition as contained in Commission-approved Reliability Standards.

(vi) *Total transfer capability* or *TTC* means the amount of electric power that can be moved or transferred reliably from one area to another area of the interconnected transmission systems by way of all transmission lines (or paths) between those areas under specified system conditions, or such definition as contained in Commission-approved Reliability Standards.

(vii) *Capacity Benefit Margin* or *CBM* means the amount of TTC preserved by the Transmission Provider for load-serving entities, whose loads are located on that Transmission Provider's system, to enable access by the load-serving entities to generation from interconnected systems to meet generation reliability requirements, or such definition as contained in Commission-approved Reliability Standards.

(viii) *Transmission Reliability Margin* or *TRM* means the amount of TTC necessary to provide reasonable assurance that the interconnected transmission network will be secure, or such definition as contained in Commission-approved Reliability Standards.

(2) *Calculation methods, availability of information, and requests.* (i) Information used to calculate any posting of ATC and TTC must be dated and time-stamped and all calculations shall be performed according to consistently applied methodologies referenced in the Transmission Provider's transmission tariff and shall be based on Commission-approved Reliability Standards as well as current industry practices, standards and criteria.

(ii) On request, the Responsible Party must make all data used to calculate ATC, TTC, CBM, and TRM for any constrained posted paths publicly available (including the limiting element(s) and the cause of the limit ( *e.g.* , thermal, voltage, stability), as well as load forecast assumptions) in electronic form within one week of the posting. The information is required to be provided only in the electronic format in which it was created, along with any necessary decoding instructions, at a cost limited to the cost of reproducing the material. This information is to be retained for six months after the applicable posting period.

(iii) System planning studies, facilities studies, and specific network impact studies performed for customers or the Transmission Provider's own network resources are to be made publicly available in electronic form on request and a list of such studies shall be posted on the OASIS. A study is required to be provided only in the electronic format in which it was created, along with any necessary decoding instructions, at a cost limited to the cost of reproducing the material. These studies are to be retained for five years.

(3) *Posting.* The ATC, TTC, CBM, and TRM for all Posted Paths must be posted in megawatts by specific direction and in the manner prescribed in this subsection.

(i) *Constrained posted paths* —(A) *For firm ATC and TTC.*

( *1* ) The posting shall show ATC, TTC, CBM, and TRM for a 30-day period. For this period postings shall be: by the hour, for the current hour and the 168 hours next following; and thereafter, by the day. If the Transmission Provider charges separately for on-peak and off-peak periods in its tariff, ATC, TTC, CBM, and TRM will be posted daily for each period.

( *2* ) Postings shall also be made by the month, showing for the current month and the 12 months next following.

( *3* ) If planning and specific requested transmission studies have been done, seasonal capability shall be posted for the year following the current year and for each year following to the end of the planning horizon but not to exceed 10 years.

(B) *For non-firm ATC and TTC.* The posting shall show ATC, TTC, CBM and TRM for a 30-day period by the hour and days prescribed under paragraph (b)(3)(i)(A)( *1* ) of this section and, if so requested, by the month and year as prescribed under paragraph (b)(3)(i)(A) ( *2* ) and ( *3* ) of this section. The posting of non-firm ATC and TTC shall show CBM as zero.

(C) *Updating posted information for constrained paths.*

( *1* ) The capability posted under paragraphs (b)(3)(i)(A) and (B) of this section must be updated when transactions are reserved or service ends or whenever the estimate for the path changes by more than 10 percent.

( *2* ) All updating of hourly information shall be made on the hour.

( *3* ) When the monthly and yearly capability posted under paragraphs (b)(3)(i)(A) and (B) of this section are updated because of a change in TTC by more than 10 percent, the Transmission Provider shall post a brief, but specific, narrative explanation of the reason for the update. This narrative should include, the specific events which gave rise to the update ( *e.g.* , scheduling of planned outages and occurrence of forced transmission outages, de-ratings of transmission facilities, scheduling of planned generation outages and occurrence of forced generation outages, changes in load forecast, changes in new facilities' in-service dates, or other events or assumption changes) and new values for ATC on the path (as opposed to all points on the network).

( *4* ) When the monthly and yearly capability posted under paragraphs (b)(3)(i)(A) and (B) of this section remain unchanged at a value of zero for a period of six months, the Transmission Provider shall post a brief, but specific, narrative explanation of the reason for the unavailability of ATC.

(ii) *Unconstrained posted paths.*

(A) Postings of firm and nonfirm ATC, TTC, CBM, and TRM shall be posted separately by the day, showing for the current day and the next six days following and thereafter, by the month for the 12 months next following. If the Transmission Provider charges separately for on-peak and off-peak periods in its tariff, ATC, TTC, CBM, and TRM will be posted separately for the current day and the next six days following for each period. These postings are to be updated whenever the ATC changes by more than 20 percent of the Path's TTC.

(B) If planning and specific requested transmission studies have been done, seasonal capability shall be posted for the year following the current year and for each year following until the end of the planning horizon but not to exceed 10 years.

(iii) *Calculation of CBM.*

(A) The Transmission Provider must reevaluate its CBM needs at least every year.

(B) The Transmission Provider must post its practices for reevaluating its CBM needs.

(iv) *Daily load.* The Transmission Provider must post on a daily basis, its load forecast, including underlying assumptions, and actual daily peak load for the prior day.

(c) *Posting Transmission Service Products and Prices.* (1) Transmission Providers must post prices and a summary of the terms and conditions associated with all transmission products offered to Transmission Customers.

(2) Transmission Providers must provide a downloadable file of their complete tariffs in the same electronic format as the tariff that is filed with the Commission. Transmission Providers also must provide a link to all of the rules, standards and practices that relate to transmission services posted on the Transmission Providers' public Web sites.

(3) Any offer of a discount for any transmission service made by the Transmission Provider must be announced to all potential customers solely by posting on the OASIS.

(4) For any transaction for transmission service agreed to by the Transmission Provider and a customer, the Transmission Provider (at the time when ATC must be adjusted in response to the transaction), must post on the OASIS (and make available for download) information describing the transaction (including: price; quantity; points of receipt and delivery; length and type of service; identification of whether the transaction involves the Transmission Provider's wholesale merchant function or any affiliate; identification of what, if any, ancillary service transactions are associated with this transmission service transaction; and any other relevant terms and conditions) and shall keep such information posted on the OASIS for at least 30 days. A record of the transaction must be retained and kept available as part of the audit log required in § 37.7.

(5) Customers choosing to use the OASIS to offer for resale transmission capacity they have purchased must post relevant information to the same OASIS as used by the Transmission Provider from whom the Reseller purchased the transmission capacity. This information must be posted on the same display page, using the same tables, as similar capability being sold by the Transmission Provider, and the information must be contained in the same downloadable files as the Transmission Provider's own available capability.

(d) *Posting Ancillary Service Offerings and Prices.* (1) Any ancillary service required to be provided or offered under the *pro forma* tariff prescribed by part 35 of this chapter must be posted with the price of that service.

(2) Any offer of a discount for any ancillary service made by the Transmission Provider must be announced to all potential customers solely by posting on the OASIS.

(3) For any transaction for ancillary service agreed to by the Transmission Provider and a customer, the Transmission Provider (at the time when ATC must be adjusted in response to an associated transmission service transaction, if any), must post on the OASIS (and make available for download) information describing the transaction (including: date and time when the agreement was entered into; price; quantity; length and type of service; identification of whether the transaction involves the Transmission Provider's wholesale merchant function or any affiliate; identification of what, if any, transmission service transactions are associated with this ancillary service transaction; and any other relevant terms and conditions) and shall keep such information posted on the OASIS for at least 30 days. A record of the transaction must be retained and kept available as part of the audit log required in § 37.7.

(4) Any other interconnected operations service offered by the Transmission Provider may be posted, with the price for that service.

(5) Any entity offering an ancillary service shall have the right to post the offering of that service on the OASIS if the service is one required to be offered by the Transmission Provider under the *pro forma* tariff prescribed by part 35 of this chapter. Any entity may also post any other interconnected operations service voluntarily offered by the Transmission Provider. Postings by customers and third parties must be on the same page, and in the same format, as postings of the Transmission Provider.

(e) *Posting specific transmission and ancillary service requests and responses* —(1) *General rules.* (i) All requests for transmission and ancillary service offered by Transmission Providers under the *pro forma* tariff, including requests for discounts, and all requests to designate or terminate a network resource, must be made on the OASIS and posted prior to the Transmission Provider responding to the request, except as discussed in paragraphs (e)(1)(ii) and (iii) of this section. The Transmission Provider must post all requests for transmission service, for ancillary service, and for the designation or termination of a network resource comparably. Requests for transmission service, ancillary service, and to designate and terminate a network resource, as well as the responses to such requests, must be conducted in accordance with the Transmission Provider's tariff, the Federal Power Act, and Commission regulations.

(ii) The requirement in paragraph (e)(1)(i) of this section, to post requests for transmission and ancillary service offered by Transmission Providers under the *pro forma* tariff, including requests for discounts, prior to the Transmission Provider responding to the request, does not apply to requests for next-hour service made during Phase I.

(iii) In the event that a discount is being requested for ancillary services that are not in support of basic transmission service provided by the Transmission Provider, such request need not be posted on the OASIS.

(iv) In processing a request for transmission or ancillary service, the Responsible Party shall post the same information as required in paragraphs (c)(4) and (d)(3) of this section, and the following information: the date and time when the request is made, its place in any queue, the status of that request, and the result (accepted, denied, withdrawn). In processing a request to designate or terminate the designation of a network resource, the Responsible Party shall post the date and time when the request is made.

(v) For any request to designate or terminate a network resource, the Transmission Provider (at the time when the request is received), must post on the OASIS (and make available for download) information describing the request (including: name of requestor, identification of the resource, effective time for the designation or termination, identification of whether the transaction involves the Transmission Provider's wholesale merchant function or any affiliate; and any other relevant terms and conditions) and shall keep such information posted on the OASIS for at least 30 days. A record of the transaction must be retained and kept available as part of the audit log required in § 37.7.

(vi) The Transmission Provider shall post a list of its current designated network resources and all network customers' current designated network resources on OASIS. The list of network resources should include the name of the resource, its geographic and electrical location, its total installed capacity, and the amount of capacity to be designated as a network resource.

(2) *Posting when a request for transmission service is denied.* (i) When a request for service is denied, the Responsible Party must provide the reason for that denial as part of any response to the request.

(ii) Information to support the reason for the denial, including the operating status of relevant facilities, must be maintained for five years and provided, upon request, to the potential Transmission Customer and the Commission's Staff.

(iii) Any offer to adjust operation of the Transmission Provider's System to accommodate the denied request must be posted and made available to all Transmission Customers at the same time.

(3) *Posting when a transaction is curtailed or interrupted.* (i) When any transaction is curtailed or interrupted, the Transmission Provider must post notice of the curtailment or interruption on the OASIS, and the Transmission Provider must state on the OASIS the reason why the transaction could not be continued or completed.

(ii) Information to support any such curtailment or interruption, including the operating status of the facilities involved in the constraint or interruption, must be maintained and made available upon request, to the curtailed or interrupted customer, the Commission's Staff, and any other person who requests it, for five years.

(iii) Any offer to adjust the operation of the Transmission Provider's system to restore a curtailed or interrupted transaction must be posted and made available to all curtailed and interrupted Transmission Customers at the same time.

(f) *Posting Transmission Service Schedules Information.* Information on transmission service schedules must be recorded by the entity scheduling the transmission service and must be available on the OASIS for download. Transmission service schedules must be posted no later than seven calendar days from the start of the transmission service.

(g) *Posting Other Transmission-Related Communications.* (1) The posting of other communications related to transmission services must be provided for by the Responsible Party. These communications may include “want ads” and “other communications” (such as using the OASIS as a Transmission-related conference space or to provide transmission-related messaging services between OASIS users). Such postings carry no obligation to respond on the part of any market participant.

(2) The Responsible Party is responsible for posting other transmission-related communications in conformance with the instructions provided by the third party on whose behalf the communication is posted. It is the responsibility of the third party requesting such a posting to ensure the accuracy of the information to be posted.

(3) Notices of transfers of personnel shall be posted as described in § 358.4(c). The posting requirements are the same as those provided in § 37.7 for audit data postings.

(4) Logs detailing the circumstances and manner in which a Transmission Provider or Responsible Party exercised its discretion under any terms of the tariff shall be posted as described in § 358.5(c)(4). The posting requirements are the same as those provided in § 37.7 for audit data postings.

(h) *Posting information summarizing the time to complete transmission service request studies.* (1) For each calendar quarter, the Responsible Party must post the set of measures detailed in paragraph (h)(1)(i) through paragraph (h)(1)(vi) of this section related to the Responsible Party's processing of transmission service request system impact studies and facilities studies. The Responsible Party must calculate and post the measures in paragraph (h)(1)(i) through paragraph (h)(1)(vi) of this section for requests for short-term firm point-to-point transmission service, requests for long-term firm point-to-point transmission service, and requests to designate a new network resource or network load. When calculating the measures in paragraph (h)(1)(i) through paragraph (h)(1)(iv) of this section, the Responsible Party may aggregate requests for short-term firm point-to-point service and requests for long-term firm point-to-point service, but must calculate and post measures separately for transmission service requests from Affiliates and transmission service requests from Transmission Customers who are not Affiliates. The Responsible Party is required to include in the calculations of the measures in paragraph (h)(1)(i) through paragraph (h)(1)(vi) of this section all studies the Responsible Party conducts of transmission service requests on another Transmission Provider's OASIS.

(i) *Process time from initial service request to offer of system impact study agreement.*

(A) Number of new system impact study agreements delivered during the reporting quarter to entities that request transmission service,

(B) Number of new system impact study agreements delivered during the reporting quarter to entities that request transmission service more than thirty (30) days after the Responsible Party received the request for transmission service,

(C) Mean time (in days), for all requests acted on by the Responsible Party during the reporting quarter, from the date when the Responsible Party received the request for transmission service to when the Responsible Party changed the transmission service request status to indicate that the Responsible Party could offer transmission service or needed to perform a system impact study,

(D) Mean time (in days), for all system impact study agreements delivered by the Responsible Party during the reporting quarter, from the date when the Responsible Party received the request for transmission service to the date when the Responsible Party delivered a system impact study agreement, and

(E) Number of new system impact study agreements executed during the reporting quarter.

(ii) *System impact study processing time.*

(A) Number of system impact studies completed by the Responsible Party during the reporting quarter,

(B) Number of system impact studies completed by the Responsible Party during the reporting quarter more than 60 days after the Responsible Party received an executed system impact study agreement,

(C) For all system impact studies completed more than 60 days after receipt of an executed system impact study agreement, average number of days study was delayed due to transmission customer's actions ( *e.g.* , delays in providing needed data),

(D) Mean time (in days), for all system impact studies completed by the Responsible Party during the reporting quarter, from the date when the Responsible Party received the executed system impact study agreement to the date when the Responsible Party provided the system impact study to the entity who executed the system impact study agreement, and

(E) Mean cost of system impact studies completed by the Responsible Party during the reporting quarter.

(iii) *Transmission service requests withdrawn from the system impact study queue.*

(A) Number of transmission service requests withdrawn from the Responsible Party's system impact study queue during the reporting quarter,

(B) Number of transmission service requests withdrawn from the Responsible Party's system impact study queue during the reporting quarter more than 60 days after the Responsible Party received the executed system impact study agreement, and

(C) Mean time (in days), for all transmission service requests withdrawn from the Responsible Party's system impact study queue during the reporting quarter, from the date the Responsible Party received the executed system impact study agreement to date when request was withdrawn from the Responsible Party's system impact study queue.

(iv) *Process time from completed system impact study to offer of facilities study.*

(A) Number of new facilities study agreements delivered during the reporting quarter to entities that request transmission service,

(B) Number of new facilities study agreements delivered during the reporting quarter to entities that request transmission service more than thirty (30) days after the Responsible Party completed the system impact study,

(C) Mean time (in days), for all facilities study agreements delivered by the Responsible Party during the reporting quarter, from the date when the Responsible Party completed the system impact study to the date when the Responsible Party delivered a facilities study agreement, and

(D) Number of new facilities study agreements executed during the reporting quarter.

(v) *Facilities study processing time.*

(A) Number of facilities studies completed by the Responsible Party during the reporting quarter,

(B) Number of facilities studies completed by the Responsible Party during the reporting quarter more than 60 days after the Responsible Party received an executed facilities study agreement,

(C) For all facilities studies completed more than 60 days after receipt of an executed facilities study agreement, average number of days study was delayed due to transmission customer's actions ( *e.g.* , delays in providing needed data),

(D) Mean time (in days), for all facilities studies completed by the Responsible Party during the reporting quarter, from the date when the Responsible Party received the executed facilities study agreement to the date when the Responsible Party provided the facilities study to the entity who executed the facilities study agreement,

(E) Mean cost of facilities studies completed by the Responsible Party during the reporting quarter, and

(F) Mean cost of upgrades recommended in facilities studies completed during the reporting quarter.

(vi) *Service requests withdrawn from facilities study queue.*

(A) Number of transmission service requests withdrawn from the Responsible Party's facilities study queue during the reporting quarter,

(B) Number of transmission service requests withdrawn from the Responsible Party's facilities study queue during the reporting quarter more than 60 days after the Responsible Party received the executed facilities study agreement, and

(C) Mean time (in days), for all transmission service requests withdrawn from the Responsible Party's facilities study queue during the reporting quarter, from the date the Responsible Party received the executed facilities study agreement to date when request was withdrawn from the Responsible Party's facilities study queue.

(2) The Responsible Party is required to post the measures in paragraph (h)(1)(i) through paragraph (h)(1)(vi) of this section for each calendar quarter within 15 days of the end of the calendar quarter. The Responsible Party will keep the quarterly measures posted on OASIS for three calendar years.

(3) The Responsible Party will be required to post on OASIS the measures in paragraph (h)(3)(i) through paragraph (h)(3)(iv) of this section in the event the Responsible Party, for two consecutive calendar quarters, completes more than twenty (20) percent of the studies associated with requests for transmission service from entities that are not Affiliates of the Responsible Party more than sixty (60) days after the Responsible Party delivers the appropriate study agreement. The Responsible Party will have to post the measures in paragraph (h)(3)(i) through paragraph (h)(3)(iv) of this section until it processes at least ninety (90) percent of all studies within 60 days after it has received the appropriate executed study agreement. For the purposes of calculating the percent of studies completed more than sixty (60) days after the Responsible Party delivers the appropriate study agreement, the Responsible Party should aggregate all system impact studies and facilities studies that it completes during the reporting quarter.

(i) Mean, across all system impact studies the Responsible Party completes during the reporting quarter, of the employee-hours expended per system impact study the Responsible Party completes during reporting period;

(ii) Mean, across all facilities studies the Responsible Party completes during the reporting quarter, of the employee-hours expended per facilities study the Responsible Party completes during reporting period;

(iii) The number of employees the Responsible Party has assigned to process system impact studies;

(iv) The number of employees the Responsible Party has assigned to process facilities studies.

(4) The Responsible Party is required to post the measures in paragraph (h)(3)(i) through paragraph (h)(3)(iv) of this section for each calendar quarter within 15 days of the end of the calendar quarter. The Responsible Party will keep the quarterly measures posted on OASIS for five calendar years.

(i) *Posting data related to grants and denials of service.* The Responsible Party is required to post data each month listing, by path or flowgate, the number of transmission service requests that have been accepted and the number of transmission service requests that have been denied during the prior month. This posting must distinguish between the length of the service request ( *e.g.* , short-term or long-term requests) and between the type of service requested ( *e.g.* , firm point-to-point, non-firm point-to-point or network service). The posted data must show:

(1) The number of non-Affiliate requests for transmission service that have been rejected,

(2) The total number of non-Affiliate requests for transmission service that have been made,

(3) The number of Affiliate requests for transmission service, including requests by the transmission provider's merchant function to designate a network resource or to procure secondary network service, that have been rejected, and

(4) The total number of Affiliate requests for transmission service, including requests by the transmission provider's merchant function to designate, or terminate the designation of, a network resource or to procure secondary network service, that have been made.

(j) *Posting redispatch data.*

(1) The Transmission Provider must allow the posting on OASIS of any third party offer to relieve a specified congested transmission facility.

(2) The Transmission Provider must post on OASIS (i) its monthly average cost of planning and reliability redispatch, for which it invoices customers, at each internal transmission facility or interface over which it provides redispatch service and (ii) a high and low redispatch cost for the month for each of these same transmission facilities. The transmission provider must post this data on OASIS as soon as practical after the end of each month, but no later than when it sends invoices to transmission customers for redispatch-related services.

**§ 37.7 Auditing Transmission Service Information.**

(a) All OASIS database transactions, except other transmission-related communications provided for under § 37.6(g)(2), must be stored, dated, and time stamped.

(b) Audit data must remain available for download on the OASIS for 90 days, except ATC/TTC postings that must remain available for download on the OASIS for 20 days. The audit data are to be retained and made available upon request for download for five years from the date when they are first posted in the same electronic form as used when they originally were posted on the OASIS.