Amended sections of Part 121 under Proposed Rule “Disclosure of Seat Dimensions to Facilitate Use of Child Safety Seats on Airplanes During Passenger-Carrying Operations”

PART 121—OPERATING REQUIREMENTS: DOMESTIC, FLAG, AND SUPPLEMENTAL OPERATIONS

1. The authority citation for part 121 is revised to read as follows:

Authority: 49 U.S.C. 106(f), 106(g), 40103, 40113, 40119, 41706, 42301 preceding note added by Pub. L. 112–95, sec. 412, 126 Stat. 89, 44101, 44701–44702, 44705, 44709– 44711, 44713, 44716–44717, 44722, 46105; Pub. L. 111–216, 124 Stat. 2348 (49 U.S.C. 44701 note).

■ 2. Amend § 121.311 by adding a new paragraph (k) to read as follows:
§ 121.311 Seats, safety belts, and shoulder harnesses.

* * * * *

(k) Each air carrier that conducts operations under this part and that has a Web site must make available on its Web site the width of the widest passenger seat in each class of service for each airplane make, model and series operated by that air carrier in passenger-carrying operations.

■ 3. Amend § 121.583 by revising paragraph (a) introductory text to read as follows:

§ 121.583 Carriage of persons without compliance with the passenger-carrying requirements of this part.

(a) When authorized by the certificate holder, the following persons, but no others, may be carried aboard an airplane without complying with the passenger-carrying airplane requirements in §§ 121.309(f), 121.310, 121.311(k), 121.391, 121.571, and 121.587; the passenger-carrying operation requirements in part 117 and §§ 121.157(c) and 121.291; and the requirements pertaining to passengers in §§ 121.285, 121.313(f), 121.317, 121.547, and 121.573:
