|  |
| --- |
| **e-CFR Data is current as of February 20, 2014** |

[Browse Previous](http://www.ecfr.gov/cgi-bin/retrieveECFR?gp=&SID=130aa03080358574b73c18df14754d93&r=SECTION&n=47y1.0.1.1.18.2.239.6)

Title 47: Telecommunication   
[PART 18—INDUSTRIAL, SCIENTIFIC, AND MEDICAL EQUIPMENT](http://www.ecfr.gov/cgi-bin/retrieveECFR?gp=&SID=130aa03080358574b73c18df14754d93&n=47y1.0.1.1.18&r=PART&ty=HTML)   
[Subpart B—Applications and Authorizations](http://www.ecfr.gov/cgi-bin/retrieveECFR?gp=&SID=130aa03080358574b73c18df14754d93&n=47y1.0.1.1.18.2&r=SUBPART&ty=HTML)

**§18.213   Information to the user.**

Information on the following matters shall be provided to the user in the instruction manual or on the packaging if an instruction manual is not provided for any type of ISM equipment:

(a) The interference potential of the device or system

(b) Maintenance of the system

(c) Simple measures that can be taken by the user to correct interference.

(d) Manufacturers of RF lighting devices must provide an advisory statement, either on the product packaging or with other user documentation, similar to the following: This product may cause interference to radio equipment and should not be installed near maritime safety communications equipment or other critical navigation or communication equipment operating between 0.45-30 MHz. Variations of this language are permitted provided all the points of the statement are addressed and may be presented in any legible font or text style.

[50 FR 36069, Sept. 5, 1985, as amended at 51 FR 17970, May 16, 1986; 64 FR 37419, July 12, 1999]