**NCAP Vehicle Rating Practice**

|  |  |
| --- | --- |
| **Body Style / Trim** |  **Agency Reporting Practice** |
| **Passenger Cars** |  |
| **2-door**  | Rated separately for front, side, and rollover  |
| **4-door** | Rated separately for front, side, and rollover |
| **Hatchback**  | 5-door –Rating imputed from 4-door for front, side, and rollover 3-door –Rating imputed from 2-door for front, side, and rollover |
| **Station Wagon** | Rating imputed from 4-door for front, side, and rollover |
| **Convertible** | Rated separately for front and side Rating imputed from 2-door for rollover |
| **2WD/4WD** | Same rating for front, side, and rollover |
| **Pickups** |  |
| **2-door Cab** | Rating imputed from extended cab for front and sideRollover – Same rating for 2-door cab, extended cab and 4-door cab |
| **Extended Cab** | Rated separately for front and sideRollover – Same rating for 2-door cab, extended cab and 4-door cab |
| **4-door Cab****(Full size doors)** | Rated separately for front and sideRollover – Same rating for 2-door cab, extended cab and 4-door cab  |
| **2WD/4WD** | Same rating for front and sideRollover – Both statically tested. 4WD dynamically tested – If no tip-up, result imputed to 2WD. If tip-up, 2WD dynamically tested.  |
| **SUVs** |  |
| **2WD/4WD** | Same rating for front and sideRollover – Both statically tested. 2WD dynamically tested – If no tip-up, result imputed to 4WD. If tip-up, 4WD dynamically tested.  |
| **Vans** **(includes Minivans)** |  |
| **8-passenger** | Front – Same rating for passenger van and cargo van Side – Same rating for front seats of passenger van and cargo van Rollover – Ratings based on SSF and dynamic test.  |
| **12- and 15-passenger** | Front –12- and 15-passenger van share the same rating as the 8-passenger Side – Rated separately from 8-passenger if different wheelbaseRollover- 12- and 15-passenger vans will be rated as required by SAFETEA-LU. |

|  |  |
| --- | --- |
| **Cargo (full-sized van)** | Front – Rating is imputed from passenger van Side – Rating is imputed from front seats of passenger van No rating is given for rollover |
| **Engines and Transmissions** |  |
| **Gasoline Only** | Rated separately for front, side, and rollover |
| **Hybrid** | Rating imputed from the gasoline version for front, side, and rollover |
| **Electric** | Rated separately for front, side, and rollover |
| **Compressed Natural Gas (CNG )** | Rated separately for front, side, and rollover |
| Plug-in Hybrid Electric Vehicle **(PHEV)** | Rated separately for front, side, and rollover, if vehicle contains a Lithium-ion battery for propulsionRating imputed from gasoline version for front, side, and rollover for all other battery types |