|  |  |  |
| --- | --- | --- |
| U.S. DEPARTMENT OF HOMELAND SECURITYU.S. COAST GUARD | Nondestructive Testing of Certain Cargo Tanks on Unmanned Barges | OMB No. 1625-0052Exp: 09/30/2022 |

|  |  |
| --- | --- |
| **Who must comply?** | Owners of barges that transport liquefied flammable gases. |
| **What is this collection about?** | The Coast Guard (CG) uses the results of nondestructive testing (NDT) to evaluate the suitability of older pressure-vessel-type cargo tanks of unmanned barges to remain in service. Once every ten years a tank, on an unmanned barge, 30 years old or older must undergo NDT. |
| **Where do I find the requirements for this information?** | Title 46 CFR 38.25 is available at—<https://www.eCFR.gov>, select TITLE 46 – SHIPPING, and follow to Part 38.25. |
| **When must information be submitted to the Coast Guard?** | Before NDT is conducted, the owner shall submit a proposal to the CG Officer in Charge, Marine Inspection (OCMI) for acceptance. Within 30 days after completing the NDT, the owner shall submit a written report of the results to OCMI. |
| **How is the information submitted?** | In writing or electronically via e-mail or fax to the local OCMI. Contact info for CG OCMIs can be found at—<https://www.uscg.mil/Units/Organization/>. |
| **What happens when complete information is received?** | For a proposal, the OCMI will evaluate it to determine if the proposed NDT methods and scope are suitable for the purposes of detecting defects. The OCMI will advise the owner if the proposal is accepted or rejected. For NDT test results, the OCMI will evaluate them to assess the condition of the tanks and to evaluate the suitability of the tank for continued service. The OCMI will advise the owner if the vessel may continue in service.  |
| **For additional information, contact--** | Your local CG Sector Office. * A list of Coast Guard sectors, as part of a comprehensive list of Coast Guard units, can be found at <https://www.uscg.mil/Units/Organization/>.
 |