Special Conditions – Dugout Construction/Cleanout

1. Any additional permits and/or permission required for this action (County, State, Federal Agencies i.e. farm bill) are the responsibilities of the landowner. Permission from upstream or downstream landowners/township boards and adjacent landowners permission are the responsibilities of the landowner. The USFWS will NOT be held liable for any damages caused by this action.
2. The dugout is to be constructed in the location as shown on the attached map and/or as staked in the field. Removing additional material beyond what has been approved may result in wetland easement related violations.
3. Spoil is to be placed outside of the wetland basin, and can be leveled so long as it is not used to fill other wetland basins.
4. Side slopes should be constructed at a 3:1 ratio. USDA/NRCS specifications should be followed.
5. Future cleanout of the dugout will require an additional permit.