**Attachment for Notification of AM All-Digital Operations**

New all-digital AM notification requirements have been added to new section 73.406 of the Commission’s rules.

**9**. All-digital AM station filers must submit an attachment to the FCC 335-AM Digital Notification containing the following information:

1. For all-digital AM stations, the type of notification (all-digital notification, increase in nominal power, reduction in nominal power, transition from core-only to enhanced, transition from enhanced to core-only, reversion from all-digital to hybrid or analog operation);
2. the date that new or modified all-digital operation will commence or has ceased;
3. the nominal power of the all-digital station;

1. a certification that the all-digital operations will conform to the relevant nominal power and spectral emissions limits;

1. For all-digital AM stations, if a notification of commencement of new all-digital service or a nominal power change, whether the station is operating in core-only or enhanced mode.
2. For all-digital AM stations, a certification that the all-digital station complies with all EAS requirements.