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PURPOSE AND USE OF THIS DOCUMENT

This data set contributes to the Environmental Public Health Tracking Network. The Content Workgroup Radon Team identified nationally consistent data sources and developed a nationally consistent indicator and measures of radon in air. 
VERSION HISTORY

	Field Name
	Description 

	1.0
	May 2027: Initial version of formatted document. Combined form for Tracking recipients and radon testing labs. 



[bookmark: _Hlk96349130]ENVIRONMENTAL PUBLIC HEALTH TRACKING DATA SET SUMMARY, RADON   

	Characteristic
	Description 

	Data Source
	Radon test data from states and private labs

	Purpose
	This data set contributes to the Environmental Public Health Tracking Network. The Content Workgroup Radon Team identified nationally consistent data sources and developed a nationally consistent indicator and measures of radon in air.

	Geographic Level
	County or census tract

	Restrictions
	This is a restricted access data set.
Data will be displayed via the national public portal only when sufficient conditions have been met to protect data privacy.

	Last Revised
	May 2026

	Instruction for Use
	This data dictionary is a reference for creating the radon data for submission. Refer to the radon schema for the order of variables and final data structure. 
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Description automatically generated with medium confidence] Environmental Public Health Tracking Program
Data Dictionary

	Field Name 
	Field Description 
	Data Type
	Code Scheme
	Allowed Values 
	Field Length
	Required

	Header Information for data submitter
	Code to identify the data submitter, by state or by lab
	String
	XXX
	
Valid State FIPS code or valid code assigned by CDC Tracking
	
3
	Required (lab identifier codes will be provided to labs by CDC Tracking)

	RowIdentifier
	An identifier for each row of data
	Integer
	1 – nnnn
The maximum RowIdentifier should be equal to the number of test results submitted for that year.
	Consecutive numerical identifier for each record in the dataset. 
	N/A
	Required

	TestYear
	The year the data are assigned to, i.e., the year analysis completed
	Integer
	YYYY
	Ex: 
2018
	4
	Required

	StateFIPSCode
	State FIPS Code where test was taken
	String
	XX
	Valid state FIPS code
	2
	Required

	CountyFIPSCode
	County FIPS Code where test was taken
	String
	XXXXX;
U=Unknown
	A valid county FIPS Code for the state and county in which test was conducted
	5
	Required

	CensusTractFIPSCode			
		
	Consists of the 2- digit state FIPS code, the 3-digit county FIPS code and the 6-digit code for the census tract
	String
	XXXXXXXXXXX;
U=Unknown
	Valid 11-digit census tract FIPS 
	11
	Required

	AddressPostalCode
	5-digit zip code and 4-digit extension code (if available)
	String
	xxxxx or
xxxxx-xxxx;
U = Unknown
	Valid ZIP or ZIP+4 format, example: 
19145 or 
19145-5208
	5 or 10
	Optional 

	DataIdentifier
	A unique identifier for each batch of radon test results
	String
	XXXXXXXXX
	Nine-character value consisting of numbers or letters identifying the batch
	9
	Optional

	AddressIdentifier 
	This is a unique ID that can be linked to the address but maintain confidentiality; this number represents an address level record but it is not the address.
	String
	One hundred character value (at a maximum) consisting of numbers or letters that link to a specific address
	nnnnnn….
String of integers and characters
	100
	Required

	PropertyIdentifier
	For use in multi-family housing complex
	String
	XXXXXX;
NA
	Any number character value (up to 20) that identifies a unique test result
	20
	Required

	BuildingIdentifier
	This is a unique ID that links all tests done within the same building or structure. This could be to group tests conducted in the same single-family home or to group tests conducted in a multi-family housing complex with several structures.
	String
	XXXXXX
	Any number character value (up to 20) that identifies a unique test result
	20
	Required

	TestResultIdentifier

	A unique identifier for each lab result, there may be multiple tests per address, this number will be unique for each test
	String
	XXXXXX
	Any number character value (up to 20) that identifies a unique test result
	20
	Required

	TestStartDate
	The date the test was begun
	Integer
	YYYYMMDD; 
NC = not collected
	Ex: 
20181022
	8
	Required

	TestStopDate
	The date the test ended
	Integer
	YYYYMMDD; 
NC = not collected
	Ex: 
20181025
	8
	Required

	MeasureValue
	The actual radon measurement
	Integer 
	 nnnnn.n;
-999=LLD (less than the limit of detection)
	0-10000.5, 
-999
	5,1
	Required

	MeasureUnitName
	The code that represents the unit for measuring radon (pCi/L = picocuries per Liter). Note: look for conversion factor for working levels in How-To Guide.
	Integer
	Please report only as 1= pCi/L for Radon 

	1
	1
	Required

	TestMethodTypeCode

	Identifier of the type or category of test                                                  
	Integer
	1 = Pre-mitigation
2 = Post-mitigation
3 = Not collected
4 = Follow-up pre-mitigation
5 = Follow-up post-mitigation
	1, 2, 3, 4, 5
	3
	Required

	ReasonForTest
	The reason the radon test is being conducted
	Integer
	1=Real estate transaction
2=Homeowner’s choice (personal knowledge)
3=Legal requirement
4=Real estate transaction and legal requirement
5=Response to outreach/promotion
6=Post-mitigation test
7 = Tenant (renter) choice
8 = Other
9 = Unknown
	Any of the codes in the Code Scheme column
	1 
	Required

	RealEstateTransactionIndicator
	Indicator of the building being tested for radon due to a real estate transaction or not                                                                                                      
	Integer
	1 = Yes
0 = No
9 = Unknown
	Any of the codes in the Code Scheme column
	1
	Required

	RealEstateTransactionType

	Indicator of the building being tested for radon due to a real estate transaction and client identity

	String
	1 = Sale – seller 
2 = Sale - buyer
3 = Rental – landlord
4 = Rental – tenant
NA = Does not apply
U = Unknown

	Any of the codes in the Code Scheme column

	2
	Required

	PublicHousing
	 A designator to identify if public housing data are being submitted
	Integer
	1 = Yes 
0 = No
9 = Unknown
	0, 1
	1
	Required

	LoanFinancingSource

	The designator to identify loan underwriter or subsidy

	String
	FA = Fannie Mae
FH = HUD FHA
FR = Freddie Mac
PH = Public Housing
OH = Other HUD
P = Private 
NA = Does not apply
U = Unknown
	Any of the codes in the Code Scheme column
	2
	Required

	BuildingPurposeCode
	The designator that represents the building purpose                                
	Text
	R = Residential
N = Non-residential/commercial
C = Community water supply this is a water sample
D = Daycare center
P = Childcare/pre-school in public school
S = School (K-12)
H= Hospital/other healthcare
G = Government building
E = Colleges, universities, or other higher education
I = Institutional
U = Unknown  
	 
Any of the codes in Code Scheme column
	2
	Required

	HousingType
	The designator that clearly identifies whether multi-family housing data are being submitted
	Text
	SF = Single family
MF = Multi-family
NR = Non-residential
U = Unknown
	Any of the codes in the Code Scheme column
	2
	Required

	FloorLevelTested
	The floor level in the building where the radon test was conducted
	String
	B = Basement
F1 = 1st floor
F2 = 2nd floor
F3 = 3rd floor
F4 = 4th floor
O = Other
U = Unknown
	Any of the codes in the Code Scheme column
	2
	Required

	GroundContact

	The designator identifies whether unit is in contact with ground or above unoccupied or crawl space

	Integer
	1 = Yes
0 = No
9 = Unknown
	Any of the codes in the Code Scheme column
	1
	Required

	GroundContactUnits

	The number of ground contact units in the building. Use only for large scale multifamily housing testing.

	String
	XXX;
NA = Does not apply

	Any of the codes in the Code Scheme column
	3
	Required

	FoundationTypeCode
	A designator used to uniquely identify the Foundation Type that facility occupies                                                                                                       
	Text
	B = Basement
C = Crawlspace
S = Slab-on-grade
P = Pier
K= Skirted in pier
O = Other
U = Unknown
	Any of the codes in the Code Scheme column
	1
	Required

	TestDeviceLocation

	Specific room in the house where the Radon test was conducted                                                                                                                                  
	Text
	BR = Bedroom
BA = Basement
CL = Classroom
NR = Non-residential/commercial
HC = Healthcare
O = Other
U = Unknown
	Any of the codes in the Code Scheme column
	2
	Required


	TestConditions 
	The designator identifies the observed test conditions for the building at test start

	String
	1 = Closed building
2 = Not closed building
3 = Unknown

	Values in code scheme column 

	1
	Required

	WeatherConditions

	Identifies anomalous weather conditions during short term tests   

	String
	1 = Normal
2 = Severe conditions
3 = Extreme temperatures
4 = Severe conditions and extreme temperatures
5 = Unknown
	Values in code scheme column 

	1
	Required

	MultipleTests

	Indicator of unique test per unit/room, average, or reason for more than one test result per unit 

	String
	0 = Unique test 
1 = Collocated
2 = In same unit but not collocated 
9 = Unknown
	Values in code scheme column 

	1
	Required

	DeviceTypeName
	Name of instrument or equipment used for the radon test 
	String
	AT = Alpha Track 
CA = Charcoal Adsorption
EI = Electret Ion Chamber
LS = Liquid Scintillation
CR = Continuous Radon Monitor
O = Other
U = Unknown
	Any of the codes in the Code Scheme column
	2
	Required

	TestingProtocol
	Identify primary testing protocol used to perform radon measurement

	Integer
	1 = ANSI-AARST Standards
2 = State-specific protocols
3 = Lender-specific protocols
4 = Manufacturer’s instructions 
	Values in code scheme column

	1
	Required

	TestPerformer

	Indicator of the role of the person performing the test

	Integer
	1 = Homeowner/tenant 
2 = Both certified by an EPA-recognized program and state-credentialed for radon measurement
3 = Certified by an EPA-recognized program
4 = State-credentialed for radon measurement
0 = Other
	Values in code scheme column

	1
	Required

	MitigationSystem

	The designator that clearly identifies whether mitigation system exists and is operational

	Integer
	1 = Yes – Active, fan and manometer operational
2 = Yes – Active, status unknown
3 = Yes – Passive
4 = No

	Values in code scheme column

	1
	Required
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Contact us: trackingsupport@cdc.gov 
Visit the Tracking Network today: www.cdc.gov/ephtracking 
Follow us on social media:
· X (@CDC_EPHTracking) 
· Facebook (facebook.com/CDCEPHTracking)
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