FERC-725S (OMB# 1902-0270)

Supporting Statement for
FERC-725S (Mandatory Reliability Standards: Emergency Preparedness 
and Operations (EOP) Reliability Standards)

The Federal Energy Regulatory Commission (Commission or FERC) requests that the Office of Management and Budget (OMB) review and approve FERC-725S (Mandatory Reliability Standards: Emergency Preparedness and Operations (EOP) Reliability Standards) under OMB Control No. 1902-0270 for a three-year period. 

1. CIRCUMSTANCES THAT MAKE THE COLLECTION OF INFORMATION NECESSARY

Background.  On August 8, 2005, The Electricity Modernization Act of 2005, which is Title XII of the Energy Policy Act of 2005[footnoteRef:2] (EPAct 2005), was enacted into law.   EPAct 2005 added a new section 215 to the Federal Power Act (FPA),[footnoteRef:3] which requires a Commission-certified Electric Reliability Organization (ERO) to develop mandatory and enforceable Reliability Standards, subject to Commission review and approval.  Once approved, the Reliability Standards may be enforced by the ERO, subject to Commission oversight, or by the Commission independently. In 2006, the Commission certified North American Electric Reliability Corporation (NERC) as the ERO pursuant to section 215 of the FPA.  [2:  16 U.S.C. 824d(a)]  [3:  16 U.S.C. 824o.  The approved Reliability Standards are available on the Commission’s eLibrary document retrieval system in Docket No. RM17-12-000 and on the NERC website, www.nerc.com.  ] 


Pursuant to section 215 of the Federal Power Act (FPA),[footnoteRef:4] the Commission has approved Emergency Preparedness and Operations (EOP) Reliability Standards EOP-004-4 (Event Reporting), EOP-005-3 (System Restoration from Blackstart Resources), EOP-006-3 (System Restoration Coordination), and EOP-008-2 (Loss of Control Center Functionality), submitted by the North American Electric Reliability Corporation (NERC), the Commission-certified Electric Reliability Organization (ERO).  The Commission also approved the associated violation risk factors, violation severity levels, implementation plans, and effective dates of the Reliability standards EOP-004-4, EOP-005-3, EOP-006-3 and EOP-008-2, EOP-010-1, and EOP-011-1.  [4:  16 U.S.C. 824o.  ] 





2.  HOW, BY WHOM, AND FOR WHAT PURPOSE THE INFORMATION IS TO BE USED AND THE CONSEQUENCES OF NOT COLLECTING THE INFORMATION

[bookmark: _Hlk55404923][bookmark: _Hlk61359837]FERC-725S consists of Emergency Preparedness and Operations (EOP) Reliability Standards, EOP-004-4 (Event Reporting), EOP-005-3 (System Restoration from Blackstart Resources), EOP-006-3 (System Restoration Coordination), and EOP-008-2 (Loss of Control Center Functionality), EOP-010-1 (Geomagnetic Disturbance Operations), and EOP-011-1 (Emergency Operations).  These Reliability Standards enhance reliability by:  
1) providing accurate reporting of events to NERC’s event analysis group to analyze the impact on the reliability of the bulk electric system (Reliability Standard EOP-004-4). 
2) delineating the roles and responsibilities of entities that support system restoration from blackstart resources which generate power without the support of the bulk electric system (Reliability Standard EOP-005-3).
3) clarifying the procedures and coordination requirements for reliability coordinator personnel to execute system restoration processes (Reliability Standard EOP-006-3).
4) refining the required elements of an operating plan used to continue reliable operations of the bulk electric system in the event that primary control center functionality is lost (Reliability Standard EOP-008-2).
5) addressing the effects of operating Emergencies by ensuring each Transmission Operator and Balancing Authority has developed Operating Plan(s) to mitigate operating Emergencies, and that those plans are coordinated within a Reliability Coordinator Area (EOP-010-1).
6) streamlining the requirements for Emergency operations of the Bulk Electric
System. Attachment 1, which is incorporated into Requirements R2 and R6, provides the process and descriptions of the levels used by the Reliability Coordinator when communicating the condition of a Balancing Authority that is experiencing an Energy Emergency (EOP-011-1).

EOP-004-4 Requirements and Measures 

R1. Each Responsible Entity shall have an event reporting Operating Plan in accordance with EOP-004-4 Attachment 1 that includes the protocol(s) for reporting to the Electric Reliability Organization and other organizations (e.g., the Regional Entity, company personnel, the Responsible Entity’s Reliability Coordinator, law enforcement, or governmental authority). 
M1. Each Responsible Entity will have a dated event reporting Operating Plan that includes protocol(s) and each organization identified to receive an event report for event types specified in EOP-004-4 Attachment 1 and in accordance with the entity responsible for reporting. 
R2. Each Responsible Entity shall report events specified in EOP-004-4 Attachment 1 to the entities specified per their event reporting Operating Plan by the later of 24 hours of recognition of meeting an event type threshold for reporting or by the end of the Responsible Entity’s next business day (4 p.m. local time will be considered the end of the business day). 
M2. Each Responsible Entity will have as evidence of reporting an event to the entities specified per their event reporting Operating Plan either a copy of the completed EOP-004-4 Attachment 2 form or a DOE-OE-417 form; and some evidence of submittal (e.g., operator log or other operating documentation, voice recording, electronic mail message, or confirmation of facsimile) demonstrating that the event report was submitted by the later of 24 hours of recognition of meeting an event type threshold for reporting or by the end of the Responsible Entity’s next business day (4 p.m. local time will be considered the end of the business day). 

EOP-004-4 Evidence Retention 

The Responsible Entity shall keep data or evidence to show compliance as identified below unless directed by its Compliance Enforcement Authority to retain specific evidence for a longer period of time as part of an investigation. 

The following evidence retention periods identify the period of time an entity is required to retain specific evidence to demonstrate compliance. For instances where the evidence retention period specified below is shorter than the time since the last audit, the Compliance Enforcement Authority may ask an entity to provide other evidence to show that it was compliant for the full time period since the last audit. 
· Each Responsible Entity shall retain the current Operating Plan plus each version issued since the last audit for Requirement R1, and Measure M1. 
· Each Responsible Entity shall retain evidence of compliance since the last audit for Requirement R2 and Measure M2. 

If a Responsible Entity is found non-compliant, it shall keep information related to the non-compliance until mitigation is complete and approved or for the duration specified above, whichever is longer. The Compliance Enforcement Authority shall keep the last audit records and all requested and submitted subsequent audit records.

EOP-005-3 Requirements and Measures 

R1. Each Transmission Operator shall develop and implement a restoration plan approved by its Reliability Coordinator. The restoration plan shall be implemented to restore the Transmission Operator’s System following a Disturbance in which one or more areas of the Bulk Electric System (BES) shuts down and the use of Blackstart Resources is required to restore the shutdown area to a state whereby the choice of the next Load to be restored is not driven by the need to control frequency or voltage regardless of whether the Blackstart Resource is located within the Transmission Operator’s System. 
M1. Each Transmission Operator shall have a dated, documented System restoration plan developed in accordance with Requirement R1 that has been approved by its Reliability Coordinator as shown with the documented approval from its Reliability Coordinator and will have evidence, such as operator logs, voice recordings or other operating documentation, voice recordings or other communication documentation to show that its restoration plan was implemented for times when a Disturbance has occurred, in accordance with Requirement R1. 
R2. Each Transmission Operator shall provide the entities identified in its approved restoration plan with a description of any changes to their roles and specific tasks prior to the effective date of the plan. 
M2. Each Transmission Operator shall have evidence such as dated electronic receipts or registered mail receipts that it provided the entities identified in its approved restoration plan with a description of any changes to their roles and specific tasks prior to the effective date of the plan in accordance with Requirement R2. 
R3. Each Transmission Operator shall review its restoration plan and submit it to its Reliability Coordinator annually on a mutually agreed, predetermined schedule. 
M3. Each Transmission Operator shall have documentation such as a dated review signature sheet, revision histories, dated electronic receipts, or registered mail receipts, that it has annually reviewed and submitted the Transmission Operator’s restoration plan to its Reliability Coordinator in accordance with Requirement R3. 
R4. Each Transmission Operator shall submit its revised restoration plan to its Reliability Coordinator for approval, when the revision would change its ability to implement its restoration plan. 
M4. Each Transmission Operator shall have documentation such as dated review signature sheets, revision histories, dated electronic receipts, or registered mail receipts, that it has submitted the revised restoration plan to its Reliability Coordinator in accordance with Requirement R4. 
R5. Each Transmission Operator shall have a copy of its latest Reliability Coordinator approved restoration plan within its primary and backup control rooms so that it is available to all of its System Operators prior to its effective date. 
M5. Each Transmission Operator shall have documentation that it has made the latest Reliability Coordinator approved copy of its restoration plan, in electronic or hardcopy format, in its primary and backup control rooms and available to its System Operators prior to its effective date in accordance with Requirement R5. 
R6. Each Transmission Operator shall verify through analysis of actual events, a combination of steady state and dynamic simulations, or testing that its restoration plan accomplishes its intended function. This shall be completed at least once every five years. 
M6. Each Transmission Operator shall have documentation, such as power flow outputs, that it has verified that its latest restoration plan will accomplish its intended function in accordance with Requirement R6. 
R7. Each Transmission Operator shall have Blackstart Resource testing requirements to verify that each Blackstart Resource is capable of meeting the requirements of its restoration plan. 
M7. Each Transmission Operator shall have documented Blackstart Resource testing requirements in accordance with Requirement R7. 
R8. Each Transmission Operator shall include within its operations training program, annual System restoration training for its System Operators. This training program shall include training on the following: 
M8. Each Transmission Operator shall have an electronic or hard copy of the training program material provided for its System Operators for System restoration training in accordance with Requirement R8. 
R9. Each Transmission Operator, each applicable Transmission Owner, and each applicable Distribution Provider shall provide a minimum of two hours of System restoration training every two calendar years to their field switching personnel identified as performing unique tasks associated with the Transmission Operator’s restoration plan that are outside of their normal tasks. 
M9. Each Transmission Operator, each applicable Transmission Owner, and each applicable Distribution Provider shall have an electronic or hard copy of the training program material provided to their field switching personnel for System restoration training and the corresponding training records including training dates and duration in accordance with Requirement R9 
R10. Each Transmission Operator shall participate in its Reliability Coordinator’s restoration drills, exercises, or simulations as requested by its Reliability Coordinator. 
M10. Each Transmission Operator shall have evidence that it participated in its Reliability Coordinator’s restoration drills, exercises, or simulations as requested in accordance with Requirement R10. 
R11. Each Transmission Operator and each Generator Operator with a Blackstart Resource shall have written Blackstart Resource Agreements or mutually agreed upon procedures or protocols, specifying the terms and conditions of their arrangement. Such Agreements shall include references to the Blackstart Resource testing requirements. 
M11. Each Transmission Operator and Generator Operator with a Blackstart Resource shall have the dated Blackstart Resource Agreements or mutually agreed upon procedures or protocols in accordance with Requirement R11. 
R12. Each Generator Operator with a Blackstart Resource shall have documented procedures for starting each Blackstart Resource and energizing a bus. 
M12. Each Generator Operator with a Blackstart Resource shall have dated documented procedures on file for starting each unit and energizing a bus in accordance with Requirement R12. 
R13. Each Generator Operator with a Blackstart Resource shall notify its Transmission Operator of any known changes to the capabilities of that Blackstart Resource affecting the ability to meet the Transmission Operator’s restoration plan within 24 hours following such change. 
M13. Each Generator Operator with a Blackstart Resource shall provide evidence, such as dated electronic receipts or registered mail receipts, showing that it notified its Transmission Operator of any known changes to its Blackstart Resource capabilities within 24 hours of such changes in accordance with Requirement R13. 
R14. Each Generator Operator with a Blackstart Resource shall perform Blackstart Resource tests, and maintain records of such testing, in accordance with the testing requirements set by the Transmission Operator to verify that the Blackstart Resource can perform as specified in the restoration plan. 
M14. Each Generator Operator with a Blackstart Resource shall maintain dated documentation of its Blackstart Resource test results and shall have evidence such as e-mails with receipts or registered mail receipts, that it provided these records to its Reliability Coordinator and Transmission Operator when requested in accordance with Requirement R14. 
R15. Each Generator Operator with a Blackstart Resource shall provide a minimum of two hours of training every two calendar years to each of its operating personnel responsible for the startup of its Blackstart Resource generation units and energizing a bus. The training program shall include training on the following.
M15. Each Generator Operator with a Blackstart Resource shall have an electronic or hard copy of the training program material provided to its operating personnel responsible for the startup, energizing a bus and synchronization of its Blackstart Resource generation units and a copy of its dated training records including training dates and durations showing that it has provided training in accordance with Requirement R15. 
R16. Each Generator Operator shall participate in its Reliability Coordinator’s restoration drills, exercises, or simulations as requested by its Reliability Coordinator. 
M16. Each Generator Operator shall have evidence that it participated in its Reliability Coordinator’s restoration drills, exercises, or simulations if requested to do so in accordance with Requirement R16. 

EOP-005-3 Evidence Retention 

The following evidence retention period(s) identify the period of time an entity is required to retain specific evidence to demonstrate compliance. For instances where the evidence retention period specified below is shorter than the time since the last audit, the Compliance Enforcement Authority may ask an entity to provide other evidence to show that it was compliant for the full-time period since the last audit.

The applicable entity shall keep data or evidence to show compliance as identified below unless directed by its Compliance Enforcement Authority to retain specific evidence for a longer period of time as part of an investigation. 

The Transmission Operator shall keep data or evidence to show compliance as identified below unless directed by its Compliance Enforcement Authority to retain specific evidence for a longer period of time as part of an investigation: 
· Approved restoration plan and any restoration plans in effect since the last compliance audit for Requirement R1, Measure M1. 
· Provided the entities identified in its approved restoration plan with a description of any changes to their roles and specific tasks prior to the effective date of the plan for the current calendar year and three prior calendar years for Requirement R2, Measure M2. 
· Submission of the Transmission Operator’s annually-reviewed restoration plan to its Reliability Coordinator for the current calendar year and three prior calendar years for Requirement R3, Measure M3. 
· Submission of a revised restoration plan to its Reliability Coordinator for all versions for the current calendar year and the prior three calendar years for Requirement R4, Measure M4. 
· The current restoration plan approved by its Reliability Coordinator and any restoration plans for the last three calendar years that was made available in its control rooms for Requirement R5, Measure M5. 
· The verification results for the current, approved restoration plan and the previous approved restoration plan for Requirement R6, Measure M6. 
· The verification process and results for the current Blackstart Resource testing requirements and the last previous Blackstart Resource testing requirements for Requirement R7, Measure M7. 
· Training program materials or descriptions for three calendar years for Requirement R8, Measure M8. 
· Records of participation in all requested Reliability Coordinator restoration drills, exercises, or simulations since its last compliance audit, as well as one previous compliance audit period for Requirement R10, Measure M10. 
· If a Transmission Operator is found non-compliant for any requirement, it shall keep information related to the non-compliance until mitigation is complete and approved or for the time period specified above, whichever is longer. The Transmission Operator, applicable Transmission Owner, and applicable Distribution Provider shall keep data or evidence to show compliance as identified below unless directed by its Compliance Enforcement Authority to retain specific evidence for a longer period of time as part of an investigation: 
· Training program materials or descriptions and training records for three calendar years for Requirement R9, Measure M9. 
· If a Transmission Operator, applicable Transmission Owner, or applicable Distribution Provider is found non-compliant for any requirement, it shall keep information related to the non-compliance until mitigation is complete and approved or for the time period specified above, whichever is longer. . 
· The Transmission Operator and Generator Operator with a Blackstart Resource shall keep data or evidence to show compliance as identified below unless directed by its Compliance Enforcement Authority to retain specific evidence for a longer period of time as part of an investigation: 
· Current Blackstart Resource Agreements and any Blackstart Resource Agreements or mutually agreed upon procedures or protocols in effect since its last compliance audit for Requirement R11, Measure M11. 
· The Generator Operator with a Blackstart Resource shall keep data or evidence to show compliance as identified below unless directed by its Compliance Enforcement Authority to retain specific evidence for a longer period of time as part of an investigation: 
· Current documentation and any documentation in effect since its last compliance audit on procedures to start each Blackstart Resource and for energizing a bus for Requirement R12, Measure M12. 
· Notification to its Transmission Operator of any known changes to its Blackstart Resource capabilities over the last three calendar years for Requirement R13, Measure M13. 
· The verification test results for the current set of requirements and one previous set for its Blackstart Resources for Requirement R14, Measure M14. 
· Training program materials and training records for three calendar years for Requirement R15, Measure M15. 
· If a Generation Operator with a Blackstart Resource is found non-compliant for any requirement, it shall keep information related to the non-compliance until mitigation is complete and approved or for the time period specified above, whichever is longer. 
· The Generator Operator shall keep data or evidence to show compliance as identified below unless directed by its Compliance Enforcement Authority to retain specific evidence for a longer period of time as part of an investigation: 
· Records of participation in all requested Reliability Coordinator restoration drills, exercises, or simulations since its last compliance audit for Requirement R16, Measure M1 
 If a Generation Operator is found non-compliant for any requirement, it shall keep information related to the non-compliance until mitigation is complete and approved or for the time period specified above, whichever is longer. The Compliance Enforcement Authority shall keep the last compliance audit records and all requested and submitted subsequent compliance audit records.

EOP-006-3 Requirements and Measures 

R1. Each Reliability Coordinator shall develop and implement a Reliability Coordinator Area restoration plan. The scope of the Reliability Coordinator’s restoration plan starts when Blackstart Resources are utilized to re-energize a shutdown area of the Bulk Electric System (BES), or separation has occurred between neighboring Reliability Coordinators, or an energized island has been formed on the BES within the Reliability Coordinator Area. The scope of the Reliability Coordinator’s restoration plan ends when all of its Transmission Operators are interconnected and its Reliability Coordinator Area is connected to all of its neighboring Reliability Coordinator Areas. The restoration plan shall include: 
M1. Each Reliability Coordinator shall have available a dated copy of its restoration plan and will have evidence, such as operator logs or other operating documentation, voice recordings, or other communication documentation to show that its restoration plan was implemented in accordance with Requirement R1. 
R2. The Reliability Coordinator shall distribute its most recent Reliability Coordinator Area restoration plan to each of its Transmission Operators and neighboring Reliability Coordinators within 30 calendar days of creation or revision. 
M2. Each Reliability Coordinator shall provide evidence such as electronic receipts, posting to a secure website with notification to affected entities, or registered mail receipts, that its most recent restoration plan has been distributed in accordance with Requirement R2. 
R3. Each Reliability Coordinator shall review its restoration plan within 13 calendar months of the last review. 
M3. Each Reliability Coordinator shall provide evidence such as a review signature sheet, or revision histories, that it has reviewed its restoration plan within 13 calendar months of the last review in accordance with Requirement R3. 
R4. Each Reliability Coordinator shall review its neighboring Reliability Coordinator’s restoration plans and provide written notification of any conflicts discovered during that review within 60 calendar days of receipt. 
M4. Each Reliability Coordinator shall provide evidence such as dated review signature sheets or electronic receipt that it has reviewed its neighboring Reliability Coordinator’s restoration plans and resolved any conflicts within the timing requirements of Requirement R4 and Requirement R4, Part 4.1. 
R5. Each Reliability Coordinator shall review the restoration plans required by EOP-005 of the Transmission Operators within its Reliability Coordinator Area. 
M5. Each Reliability Coordinator shall provide evidence such as a dated review signature sheet or electronic receipt that it has reviewed, approved or disapproved, and notified its Transmission Operators within 30 calendar days following the receipt of the restoration plan from the Transmission Operator in accordance with Requirement R5. 
R6. Each Reliability Coordinator shall have a copy of its latest restoration plan and copies of the latest approved restoration plan of each Transmission Operator in its Reliability Coordinator Area within its primary and backup control rooms so that it is available to all of its System Operators prior to the effective date. 
M6. Each Reliability Coordinator shall have documentation such as electronic receipts that it has made the latest copy of its restoration plan and copies of the latest approved restoration plan of each Transmission Operator in its Reliability Coordinator Area available in its primary and backup control rooms and to each of its System Operators prior to the effective date in accordance with Requirement R6. 
R7. Each Reliability Coordinator shall include within its operations training program, annual System restoration training for its System Operators. This training program shall address the following: 
M7. Each Reliability Coordinator shall have an electronic copy or hard copy of its training records available showing that it has provided training in accordance with Requirement R7. 
R8. Each Reliability Coordinator shall conduct two System restoration drills, exercises, or simulations per calendar year, which shall include the Transmission Operators and Generator Operators as dictated by the particular scope of the drill, exercise, or simulation that is being conducted. 
M8. Each Reliability Coordinator shall have evidence, such as dated electronic documents, that it conducted two System restoration drills, exercises, or simulations per calendar year in accordance with Requirement R8. And each Reliability Coordinator shall have evidence that the Reliability Coordinator requested each applicable Transmission Operator and Generator Operator to participate per Requirement R8 and Requirement R8.

EOP-006-3 Evidence Retention 

The following evidence retention period(s) identify the period of time an entity is required to retain specific evidence to demonstrate compliance. For instances where the evidence retention period specified below is shorter than the time since the last audit, the Compliance Enforcement Authority may ask an entity to provide other evidence to show that it was compliant for the full-time period since the last audit. 

The applicable entity shall keep data or evidence to show compliance as identified below unless directed by its Compliance Enforcement Authority to retain specific evidence for a longer period of time as part of an investigation. 
· The current restoration plan and any restoration plans in effect since the last compliance audit for Requirement R1, Measure M1. 
· Distribution of its most recent restoration plan and any restoration plans in effect for the current calendar year and three prior calendar years for Requirement R2, Measure M2. 
· It’s reviewed restoration plan for the current review period and the last three prior review periods for Requirement R3, Measure M3. 
· Reviewed copies of neighboring Reliability Coordinator restoration plans for the current calendar year and the three prior calendar years for Requirement R4, Measure M4. 
· The reviewed restoration plans for the current calendar year and the last three prior calendar years for Requirement R5, Measure M5. 
· The current, approved restoration plan and any restoration plans in effect for the last three calendar years was made available in its control rooms for Requirement R6, Measure M6. 
· Actual training program materials or descriptions for three calendar years for Requirements R7, Measure M7. 
· Records of all Reliability Coordinator restoration drills, exercises, or simulations since its last compliance audit, as well as one previous compliance audit period for Requirement R8, Measure M8. 
If a Reliability Coordinator is found non-compliant, it shall keep information related to the non-compliance until mitigation is complete and approved or for the time period specified above, whichever is longer. 

The Compliance Enforcement Authority shall keep the last audit records and all requested and submitted subsequent audit records.

EOP-008-2 Requirements and Measures 

R1. Each Reliability Coordinator, Balancing Authority, and Transmission Operator shall have a current Operating Plan describing the manner in which it continues to meet its functional obligations with regard to the reliable operations of the BES in the event that its primary control center functionality is lost. This Operating Plan for backup functionality shall include:
M1. Each Reliability Coordinator, Balancing Authority, and Transmission Operator shall have a dated, current, and in effect Operating Plan for backup functionality in accordance with Requirement R1, in electronic or hardcopy format. 
R2. Each Reliability Coordinator, Balancing Authority, and Transmission Operator shall have a copy of its current Operating Plan for backup functionality available at its primary control center and at the location providing backup functionality. 
M2. Each Reliability Coordinator, Balancing Authority, and Transmission Operator shall have a dated, current, and in effect copy of its Operating Plan for backup functionality in accordance with Requirement R2, in electronic or hardcopy format, available at its primary control center and at the location providing backup functionality. 
R3. Each Reliability Coordinator shall have a backup control center facility (provided through its own dedicated backup facility or at another entity’s control center staffed with certified Reliability Coordinator operators when control has been transferred to the backup facility) that provides the functionality required for maintaining compliance with all Reliability Standards are applicable to the primary control center functionality. To avoid requiring a tertiary facility, a backup facility is not required during: 
· Planned outages of the primary or backup facilities of two weeks or less 
· Unplanned outages of the primary or backup facilities 
M3. Each Reliability Coordinator shall provide dated evidence that it has a backup control center facility (provided through its own dedicated backup facility or at another entity’s control center staffed with certified Reliability Coordinator operators when control has been transferred to the backup facility) that provides the functionality required for maintaining compliance with all Reliability Standards that are applicable to the primary control center functionality in accordance with Requirement R3. 
R4. Each Balancing Authority and Transmission Operator shall have backup functionality (provided either through a facility or contracted services staffed by applicable certified operators when control has been transferred to the backup functionality location) that includes monitoring, control, logging, and alarming sufficient for maintaining compliance with all Reliability Standards that are applicable to a Balancing Authority’s and Transmission Operator’s primary control center functionality. To avoid requiring tertiary functionality, backup functionality is not required during: 
· Planned outages of the primary or backup functionality of two weeks or less 
· Unplanned outages of the primary or backup functionality 
M4. Each Balancing Authority and Transmission Operator shall provide dated evidence that its backup functionality (provided either through a facility or contracted services staffed by applicable certified operators when control has been transferred to the backup functionality location) includes monitoring, control, logging, and alarming sufficient for maintaining compliance with all Reliability Standards that are applicable to a Balancing Authority’s or Transmission Operator’s primary control center functionality in accordance with Requirement R4. 
R5. Each Reliability Coordinator, Balancing Authority, and Transmission Operator, shall annually review and approve its Operating Plan for backup functionality. 
M5. Each Reliability Coordinator, Balancing Authority, and Transmission Operator shall have evidence that its dated, current, and in effect Operating Plan for backup functionality, in electronic or hardcopy format, has been reviewed and approved annually and that it has been updated within sixty calendar days of any changes to any part of the Operating Plan described in Requirement R1 in accordance with Requirement R5. 
R6. Each Reliability Coordinator, Balancing Authority, and Transmission Operator shall have primary and backup functionality that do not depend on each other for the control center functionality required to maintain compliance with Reliability Standards. 
M6. Each Reliability Coordinator, Balancing Authority, and Transmission Operator shall have dated evidence that its primary and backup functionality do not depend on each other for the control center functionality required to maintain compliance with Reliability Standards in accordance with Requirement R6. 
R7. Each Reliability Coordinator, Balancing Authority, and Transmission Operator shall conduct and document results of an annual test of its Operating Plan that demonstrates: 
M7. Each Reliability Coordinator, Balancing Authority, and Transmission Operator shall provide evidence such as dated records, that it has completed and documented its annual test of its Operating Plan for backup functionality, in accordance with Requirement R7. 
R8. Each Reliability Coordinator, Balancing Authority, and Transmission Operator that has experienced a loss of its primary or backup functionality and that anticipates that the loss of primary or backup functionality will last for more than six calendar months shall provide a plan to its Regional Entity within six calendar months of the date when the functionality is lost, showing how it will re-establish primary or backup functionality. 
M8. Each Reliability Coordinator, Balancing Authority, and Transmission Operator that has experienced a loss of their primary or backup functionality and that anticipates that the loss of primary or backup functionality will last for more than six calendar months shall provide evidence that a plan has been submitted to its Regional Entity within six calendar months of the date when the functionality is lost showing how it will re-establish primary or backup functionality in accordance with Requirement R8.

EOP-008-2 Evidence Retention

The following evidence retention period(s) identify the period of time an entity is required to retain specific evidence to demonstrate compliance. For instances where the evidence retention period specified below is shorter than the time since the last audit, the Compliance Enforcement Authority may ask an entity to provide other evidence to show that it was compliant for the full-time period since the last audit. 

The applicable entity shall keep data or evidence to show compliance as identified below unless directed by its Compliance Enforcement Authority to retain specific evidence for a longer period of time as part of an investigation. 
· Each Reliability Coordinator, Balancing Authority, and Transmission Operator shall retain its dated, current, in effect Operating Plan for backup functionality plus all issuances of the Operating Plan for backup functionality since its last compliance audit in accordance with Measurement M1. 
· Each Reliability Coordinator, Balancing Authority, and Transmission Operator shall retain a dated, current, in effect copy of its Operating Plan for backup functionality, with evidence of its last issue, available at its primary control center and at the location providing backup functionality, for the current year, in accordance with Measurement M2. 
· Each Reliability Coordinator shall retain dated evidence for the time period since its last compliance audit, that it has demonstrated that it has a backup control center facility (provided through its own dedicated backup facility or at another entity’s control center staffed with certified Reliability Coordinator operators when control has been transferred to the backup facility) in accordance with Requirement R3 that provides the functionality required for maintaining compliance with all Reliability Standards that are applicable to the primary control center functionality in accordance with Measurement M3. 
· Each Balancing Authority and Transmission Operator shall retain dated evidence for the time period since its last compliance audit, that it has demonstrated that it’s backup functionality (provided either through a facility or contracted services staffed by applicable certified operators when control has been transferred to the backup functionality location) in accordance with Requirement R4 includes monitoring, control, logging, and alarming sufficient for maintaining compliance with all Reliability Standards that are applicable to a Balancing Authority’s and Transmission Operator’s primary control center functionality in accordance with Measurement M4. 
· Each Reliability Coordinator, Balancing Authority, and Transmission Operator, shall retain evidence for the time period since its last compliance audit, that its dated, current, in effect Operating Plan for backup functionality, has been reviewed and approved annually and that it has been updated within sixty calendar days of any changes to any part of the Operating Plan described in Requirement R1 in accordance with Measurement M5. 
· Each Reliability Coordinator, Balancing Authority, and Transmission Operator shall retain dated evidence for the current year and for any Operating Plan for backup functionality in effect since its last compliance audit, that its primary and backup functionality do not depend on each other for the control center functionality required to maintain compliance with Reliability Standards in accordance with Measurement M6. 
· Each Reliability Coordinator, Balancing Authority, and Transmission Operator shall retain evidence for the current calendar year and the previous calendar years, such as dated records, that it has tested its Operating Plan for backup functionality, in accordance with Measurement M7. 
· Each Reliability Coordinator, Balancing Authority, and Transmission Operator that has experienced a loss of their primary or backup functionality and that anticipates that the loss of primary or backup functionality would last for more than six calendar months shall retain evidence for the current in effect document and any such documents in effect since its last compliance audit that a plan has been submitted to its Regional Entity within six calendar months of the date when the functionality is lost showing how it will re-establish primary or backup functionality in accordance with Measurement M8 

EOP-010-1 Requirements and Measures 

R1. Each Reliability Coordinator shall develop, maintain, and implement a GMD Operating Plan that coordinates GMD Operating Procedures or Operating Processes within its Reliability Coordinator Area. At a minimum, the GMD Operating Plan shall include: 
M1. Each Reliability Coordinator shall have a current GMD Operating Plan meeting all the provisions of Requirement R1; evidence such as a review or revision history to indicate that the GMD Operating Plan has been maintained; and evidence to show that the plan was implemented as called for in its GMD Operating Plan, such as dated operator logs, voice recordings, or voice transcripts. 
R2. Each Reliability Coordinator shall disseminate forecasted and current space weather information to functional entities identified as recipients in the Reliability Coordinator's GMD Operating Plan. 
M2. Each Reliability Coordinator shall have evidence such as dated operator logs, voice recordings, transcripts, or electronic communications to indicate that forecasted and current space weather information was disseminated as stated in its GMD Operating Plan. 
R3. Each Transmission Operator shall develop, maintain, and implement a GMD Operating Procedure or Operating Process to mitigate the effects of GMD events on the reliable operation of its respective system. At a minimum, the Operating Procedure or Operating Process shall include: 
M3. Each Transmission Operator shall have a GMD Operating Procedure or Operating Process meeting all the provisions of Requirement R3; evidence such as a review or revision history to indicate that the GMD Operating Procedure or Operating Process has been maintained; and evidence to show that the Operating Procedure or Operating Process was implemented as called for in its GMD Operating Procedure or Operating Process, such as dated operator logs, voice recordings, or voice transcripts.

EOP-010-1 Evidence Retention 

The following evidence retention periods identify the period of time an entity is required to retain specific evidence to demonstrate compliance. For instances where the evidence retention period specified below is shorter than the time since the last audit, the CEA may ask an entity to provide other evidence to show that it was compliant for the full time period since the last audit. 

The Reliability Coordinator and Transmission Operator shall keep data or evidence to show compliance as identified below unless directed by its CEA to retain specific evidence for a longer period of time as part of an investigation: 
· The responsible entities shall retain documentation as evidence for three years. 
· If a responsible entity is found non-compliant, it shall keep information related to the non-compliance until mitigation is complete and approved or for the time specified above, whichever is longer. 
The CEA shall keep the last audit records and all requested and submitted subsequent audit records.

EOP-011-1 Requirements and Measures 
R1. Each Transmission Operator shall develop, maintain, and implement one or more Reliability Coordinator-reviewed Operating Plan(s) to mitigate operating Emergencies in its Transmission Operator Area. The Operating Plan(s) shall include the following, as applicable: 
M1. Each Transmission Operator will have a dated Operating Plan(s) developed in accordance with Requirement R1 and reviewed by its Reliability Coordinator; evidence such as a review or revision history to indicate that the Operating Plan(s) has been maintained; and will have as evidence, such as operator logs or other operating documentation, voice recordings or other communication documentation to show that its Operating Plan(s) was implemented for times when an Emergency has occurred, in accordance with Requirement R1. 
R2. Each Balancing Authority shall develop, maintain, and implement one or more Reliability Coordinator-reviewed Operating Plan(s) to mitigate Capacity Emergencies and Energy Emergencies within its Balancing Authority Area. The Operating Plan(s) shall include the following, as applicable: 
M2. Each Balancing Authority will have a dated Operating Plan(s) developed in accordance with Requirement R2 and reviewed by its Reliability Coordinator; evidence such as a review or revision history to indicate that the Operating Plan(s) has been maintained; and will have as evidence, such as operator logs or other operating documentation, voice recordings, or other communication documentation to show that its Operating Plan(s) was implemented for times when an Emergency has occurred, in accordance with Requirement R2. 
R3. The Reliability Coordinator shall review the Operating Plan(s) to mitigate operating Emergencies submitted by a Transmission Operator or a Balancing Authority regarding any reliability risks that are identified between Operating Plans. 
M3. The Reliability Coordinator will have documentation, such as dated e-mails or other correspondences that it reviewed Transmission Operator and Balancing Authority Operating Plans within 30 calendar days of submittal in accordance with Requirement R3. 
R4. Each Transmission Operator and Balancing Authority shall address any reliability risks identified by its Reliability Coordinator pursuant to Requirement R3 and resubmit its Operating Plan(s) to its Reliability Coordinator within a time period specified by its Reliability Coordinator. 
M4. The Transmission Operator and Balancing Authority will have documentation, such as dated emails or other correspondence, with an Operating Plan(s) version history showing that it responded and updated the Operating Plan(s) within the timeframe identified by its Reliability Coordinator in accordance with Requirement R4. 
R5. Each Reliability Coordinator that receives an Emergency notification from a Transmission Operator or Balancing Authority within its Reliability Coordinator Area shall notify, within 30 minutes from the time of receiving notification, other Balancing Authorities and Transmission Operators in its Reliability Coordinator Area, and neighboring Reliability Coordinators. 
M5. Each Reliability Coordinator that receives an Emergency notification from a Balancing Authority or Transmission Operator within its Reliability Coordinator Area will have, and provide upon request, evidence that could include, but is not limited to, operator logs, voice recordings or transcripts of voice recordings, electronic communications, or equivalent evidence that will be used to determine if the Reliability Coordinator communicated, in accordance with Requirement R5, with other Balancing Authorities and Transmission Operators in its Reliability Coordinator Area, and neighboring Reliability Coordinators . 
R6. Each Reliability Coordinator that has a Balancing Authority experiencing a potential or actual Energy Emergency within its Reliability Coordinator Area shall declare an Energy Emergency Alert, as detailed in Attachment 1. 
M6. Each Reliability Coordinator, with a Balancing Authority experiencing a potential or actual Energy Emergency within its Reliability Coordinator Area, will have, and provide upon request, evidence that could include, but is not limited to, operator logs, voice recordings or transcripts of voice recordings, electronic communications, or equivalent evidence that it declared an Energy Emergency Alert, as detailed in Attachment 1, in accordance with Requirement R6 
EOP-011-1 Evidence Retention 

The Balancing Authority, Reliability Coordinator, and Transmission Operator shall keep data or evidence to show compliance, as identified below, unless directed by its Compliance Enforcement Authority (CEA) to retain specific evidence for a longer period of time as part of an investigation. For instances where the evidence retention period specified below is shorter than the time since the last audit, the CEA may ask an entity to provide other evidence to show that it was compliant for the full time period since the last audit. 
· The Transmission Operator shall retain the current Operating Plan(s), evidence of review or revision history plus each version issued since the last audit and evidence of compliance since the last audit for Requirements R1 and R4and Measures M1 and M4. 
· The Balancing Authority shall retain the current Operating Plan(s), evidence of review or revision history plus each version issued since the last audit and evidence of compliance since the last audit for Requirements R2 and R4, and Measures M2 and M4. 
· The Reliability Coordinator shall maintain evidence of compliance since the last audit for Requirements R3, R5, and R6 and Measures M3, M5, and M6. 
If a Balancing Authority, Reliability Coordinator or Transmission Operator is found non-compliant, it shall keep information related to the non-compliance until found compliant. 
The Compliance Enforcement Authority shall keep the last audit records and all requested and submitted subsequent audit records.

3.  DESCRIBE ANY CONSIDERATION OF THE USE OF IMPROVED TECHNOLOGY TO REDUCE BURDEN AND TECHNICAL OR LEGAL OBSTACLES TO REDUCING BURDEN.
The use of current or improved technology and the medium are not covered in Reliability Standards and are therefore left to the discretion of each respondent. We think that nearly all the respondents are likely to make and keep related records in an electronic format.  Each of the six Regional Entities has a well-established compliance portal for registered entities to electronically submit compliance information and reports.  The compliance portals allow documents developed by the registered entities to be attached and uploaded to the Regional Entity’s portal.  Compliance data can also be submitted by filling out data forms on the portals.  These portals are accessible through an internet browser password-protected user interface.  

These collections do not require industry to file the information with the Commission.  However, they do contain information collection and record retention requirements for which using current technology is an option.  

4.  DESCRIBE EFFORTS TO IDENTIFY DUPLICATION AND SHOW SPECIFICALLY WHY ANY SIMILAR INFORMATION ALREADY AVAILABLE CANNOT BE USED OR MODIFIED FOR USE FOR THE PURPOSE(S) DESCRIBED IN INSTRUCTION NO. 2

The Commission periodically reviews filing requirements concurrent with OMB review or as the Commission deems necessary to eliminate duplicative filing and to minimize the filing burden.  EOP Reliability Standards do not duplicate any filing requirements.

5.  METHODS USED TO MINIMIZE THE BURDEN IN COLLECTION OF INFORMATION INVOLVING SMALL ENTITIES

In general, small entities may reduce their burden by taking part in a joint registration organization or a coordinated functional registration.  These options allow a small entity to share the compliance burden with other entities and, thus, to minimize their own compliance burden.

6.  CONSEQUENCE TO FEDERAL PROGRAM IF COLLECTION WERE CONDUCTED LESS FREQUENTLY

If the requirements of these standards were performed less frequently, NERC would not be provided any information to allow assessment of the compliance. Adequate planning for operating emergencies and responding to those emergencies is critical for the reliable operation of the bulk power system. The frequency of reporting is conducted once per year for all entities.
· Reliability Standard EOP-004-4 requires reporting of events by responsible entities. The reportable events under the proposed Reliability Standard are collected and used to examine the underlying causes of events, track subsequent corrective action to prevent recurrence of such events, and develop lessons learned for industry.  
· Reliability Standard EOP-005-3 ensures plans, facilities, and personnel are prepared to enable system restoration from blackstart resources to ensure reliability is maintained during restoration and priority is placed on restoring the Interconnection.  
· Reliability Standard EOP-006-3 establishes how personnel should prepare, execute, and coordinate system restoration processes to maintain reliability and to restore the Interconnection.  
· Reliability Standard EOP-008-2 ensures continued reliable operations of the bulk electric system if a control center becomes inoperable.  
· Reliability Standard EOP-010-1 mitigates the effects of geomagnetic disturbance (GMD) events by implementing Operating Plans, Processes, and Procedures 
· Reliability Standard EOP-011-1 addresses the effects of operating Emergencies by ensuring each Transmission Operator and Balancing Authority has developed Operating Plan(s) to mitigate operating Emergencies, and that those plans are coordinated within a Reliability Coordinator Area.

7.  EXPLAIN ANY SPECIAL CIRCUMSTANCES RELATING TO THE INFORMATION COLLECTION

The Emergency Preparedness and Operation (EOP) family of Reliability Standards represent Requirements that may need to occur in near real-time operations which if not done could place the operations of the electric system into an unknown state or lead to possible cascading, voltage instability or uncontrolled separation.  For the 30-day timeframes those were set by industry to assign responsibility to entities to communicate with others that need to plan and operate the BES in a reliable manner.

8.  DESCRIBE EFFORTS TO CONSULT OUTSIDE THE AGENCY: SUMMARIZE PUBLIC COMMENTS AND THE AGENCY'S RESPONSE TO THESE COMMENTS

Each FERC rulemaking (both proposed and final rules) is published in the Federal Register thereby providing public utilities and licensees, state commissions, Federal agencies, and other interested parties an opportunity to submit data, views, comments or suggestions concerning the proposed collections of data.  

With respect to this request for renewal of control no. 1902-0270, FERC published a public notice and invited public comment on May 20, 2026 (91 FR 29475).  The comment period ended on July 20, 2026.  The Commission received no comments.

FERC also published a public notice and invited public comment to OMB on July 21, 2026 (91 FR 45806).  

9.  EXPLAIN ANY PAYMENT OR GIFTS TO RESPONDENTS

No payments or gifts have been made to respondents.

10.  DESCRIBE ANY ASSURANCE OF CONFIDENTIALITY PROVIDED TO RESPONDENTS

According to the NERC Rules of Procedure , “…a Receiving Entity shall keep in confidence and not copy, disclose, or distribute any Confidential Information or any part thereof without the permission of the Submitting Entity, except as otherwise legally required.”  This serves to protect confidential information submitted to NERC or Regional Entities.

Responding entities do not submit the information collected due to the Reliability Standards to FERC.  Rather, they submit the information to NERC, the regional entities, or maintain it internally.  Since there are no submissions made to FERC, FERC provides no specific provisions in order to protect confidentiality.

11.  PROVIDE ADDITIONAL JUSTIFICATION FOR ANY QUESTIONS OF A SENSITIVE NATURE, SUCH AS SEXUAL BEHAVIOR AND ATTITUDES, RELIGIOUS BELIEFS, AND OTHER MATTERS THAT ARE COMMONLY CONSIDERED PRIVATE

These collections do not contain any questions of a sensitive nature.

12.  ESTIMATED BURDEN OF COLLECTION OF INFORMATION

The following table details Reliability Standards EOP-010-1, EOP-011-1, EOP-004-4, EOP-005-3, EOP-006-3, and EOP-008-2 in FERC-725S (OMB Control No. 1902-0270). The burden[footnoteRef:5] for FERC-725S reflects an increase from the previous versions of the Reliability Standards in total burden hours and cost based on adjustments in the additional entities and changes to hourly cost.[footnoteRef:6] [5:  Burden is defined as the total time, effort, or financial resources expended by persons to generate, maintain, retain, or disclose or provide information to or for a Federal agency. For further explanation of what is included in the information collection burden, refer to 5 Code of Federal Regulations 1320.3.]  [6:  The estimated hourly cost (salary plus benefits) is a combination of the following categories from the BLS website, http://www.bls.gov/​oes/​current/​naics2_​22.htm: 75% of the average of an Electrical Engineer (17-2071) $71.19/hr., × .75 = 53.3925 ($53.39-rounded) ($53.39/hour); and 25% of an Information and Record Clerk (43-4199) $40.51/hr., $40.51 × .25 = 10.1275 ($10.13 rounded) ($10.13/hour), for a total ($53.39 + $10.13 = $63.52/hour)] 



	FERC-725S
EOP-004-4 (Event Reporting)

	Reliability Standard and Associated Requirement
	Number of Respondents[footnoteRef:7][footnoteRef:8]
(1) [7:  The number of respondents is based on NERC compliance registration information as of April 20, 2026.]  [8:  For EOP-004-4 it is estimated that fifty percent of applicable entity will have an annual reporting burden and values in the table reflect that consideration (rounded up).] 

	Annual Number of Responses per Respondent
(2)
	Total Number of Responses (1) *(2) =(3)
	Average Burden & Cost Per Response
(4)
	Total Annual Burden & Total Annual Cost
(3) *(4) =(5) rounded
	Cost per Respondent
 ($)
(5) ÷(1)

	Annual review and record retention for EOP-004-4
	6 (RC)
	1
	6
	8 hrs.
$ 508.16
	48 hrs. 
$ 3,049  
	$508.16

	
	49 (BA)
	1
	49
	8 hrs.
$ 508.16
	392 hrs. 
$ 24,900   
	$508.16

	
	171 (TO)
	1
	171
	8 hrs.
$ 508.16
	1,368 hrs. 
$ 86,896   
	$508.16

	
	85 (TOP)
	1
	85
	8 hrs.
$ 508.16
	680 hrs. 
$ 43,194   
	$508.16

	
	689 (GO)
	1
	689
	8 hrs.
$ 508.16
	5,512 hrs. 
$ 350,122   
	$508.16

	
	508 (GOP)
	1
	508
	8 hrs.
$ 508.16
	4,064 hrs. 
$ 258,145   
	$508.16

	
	150 (DP)
	1
	150
	8 hrs.
$ 508.16
	1,200 hrs. 
$ 76,224   
	$508.16

	Total EOP-004-4
	
	
	
 1,658
	
	 13,264 hrs.;
$ 842,530
	



	FERC-725S
EOP-005-3 (Event Reporting)

	Reliability Standard and Associated Requirement
	Number of Respondents
(1)
	Annual Number of Responses per Respondent
(2)
	Total Number of Responses (1) *(2) =(3)
	Average Burden & Cost Per Response
(4)
	Total Annual Burden & Total Annual Cost
(3) *(4) =(5)
rounded
	Cost per Respondent
 ($)
(5) ÷(1)

	Annual review and record retention for EOP-005-3
	1,016 (GOP)
	1
	1,016
	16 hrs.
$ 1,016.32

	16,256 hrs. 
$ 1,032,581 

	$1,016.32

	
	170 (TOP)
	1
	170
	24 hrs.
$ 1,524.48
	4,080 hrs. 
$ 259,162 
	$1,524.48

	
	341 (TO)
	1
	341
	16 hrs.
$ 1,016.32
	5,456 hrs. 
$ 346,565 
	$1,016.32

	
	299 (DP)
	1
	299
	16 hrs.
$ 1,016.32
	4,784 hrs. 
$ 303,880 
	$1,016.32

	Total EOP-005-3
	
	
	1,826
	
	  30,576 hrs.
$ 1,942,188
	





	FERC-725S
EOP-006-3 (Event Reporting)

	Reliability Standard and Associated Requirement
	Number of Respondents
(1)
	Annual Number of Responses per Respondent
(2)
	Total Number of Responses (1) *(2) =(3)
	Average Burden & Cost Per Response
(4)
	Total Annual Burden & Total Annual Cost
(3) *(4) =(5)
rounded
	Cost per Respondent
 ($)
(5) ÷(1)

	Annual review and record retention for EOP-006-3
	12 (RC)
	1
	12
	48 hrs.
$ 3,048.96

	576 hrs. 
$ 36,588 

	$3,048.96

	Total EOP-006-3
	
	
	12
	
	  576 hrs.
$ 36,588
	



	FERC-725S
EOP-008-2 (Event Reporting)

	Reliability Standard and Associated Requirement
	Number of Respondents
(1)
	Annual Number of Responses per Respondent
(2)
	Total Number of Responses (1) *(2)=(3)
	Average Burden & Cost Per Response
(4)
	Total Annual Burden & Total Annual Cost
(3)*(4)=(5)
rounded
	Cost per Respondent
 ($)
(5)÷(1)

	Annual review and record retention for EOP-008-2
	12 (RC)
	1
	12
	24 hrs.;
$ 1,524.48
	288 hrs.; 
$ 18,294 
	$1524.48

	
	170 (TOP)
	1
	170
	24 hrs.;
$ 1,524.48
	4,080 hrs.; 
$ 259,162 
	$1524.48

	
	98 (BA)
	1
	98
	24 hrs.;
$ 1,524.48
	2,352 hrs.; 
$ 149,399 
	$1524.48

	Total EOP-008-2
	
	
	280
	
	6,720 hrs.;
$ 426,854
	



	FERC-725S
EOP-010-1 (Event Reporting)

	Reliability Standard and Associated Requirement
	Number of Respondents
(1)
	Annual Number of Responses per Respondent
(2)
	Total Number of Responses (1)*(2)=(3)
	Average Burden & Cost Per Response
(4)
	Total Annual Burden & Total Annual Cost
(3)*(4)=(5)
rounded
	Cost per Respondent
 ($)
(5)÷(1)

	Annual review and record retention for EOP-010-1
	12 (RC)
	1
	12
	20 hrs.;
$ 1,270.40
	240 hrs.; 
$ 15,245 
	$ 1,270.40

	
	170 (TOP)
	1
	170
	20 hrs.;
$ 1,270.40
	3,400 hrs.; 
$ 215,968
	$ 1,270.40

	Total EOP-010-1
	
	
	182
	
	3,640 hrs.;
$ 231,213
	



	FERC-725S
EOP-011-4 (Event Reporting)

	Reliability Standard and Associated Requirement
	Number of Respondents
(1)
	Annual Number of Responses per Respondent
(2)
	Total Number of Responses (1)*(2)=(3)
	Average Burden & Cost Per Response
(4)
	Total Annual Burden & Total Annual Cost
(3)*(4)=(5)
rounded
	Cost per Respondent
 ($)
(5)÷(1)

	Annual review and record retention for EOP-011-4
	12 (RC)
	1
	12
	40 hrs.;
$ 2,540.80
	480 hrs.; 
$ 30,490
	$2,540.80

	
	98 (BA)
	1
	98
	40 hrs.;
$ 2,540.80
	3,920 hrs.; 
$ 248,998 
	$2,540.80

	
	341 (TO)
	1
	341
	40 hrs.;
$ 2,540.80
	13,640 hrs.; 
$ 866,413 
	$2,540.80

	
	170 (TOP)
	1
	170
	40 hrs.;
$ 2,540.80
	6,800 hrs.; 
$ 431,936 
	$2,540.80

	
	 72 (DP-UFLS) 
	1
	72
	20 hrs.;
$ 1,270.40
	1,440 hrs.; 
$ 91,469 
	 $1,270.40

	
	299 (DP)
	1
	299
	40 hrs.;
$ 2,540.80
	11,960 hrs.; 
$ 759,699 
	$2,540.80

	Total EOP-011-4
	
	
	992
	
	  38,240 hrs.;
$ 2,429,005
	



	FERC-725S
EOP-012-3 (Event Reporting)

	Reliability Standard and Associated Requirement
	Number of Respondents
(1)
	Annual Number of Responses per Respondent
(2)
	Total Number of Responses (1)*(2)=(3)
	Average Burden & Cost Per Response
(4)
	Total Annual Burden & Total Annual Cost
(3)*(4)=(5)
	Cost per Respondent
 ($)
(5)÷(1)

	Annual review and record retention for EOP-012-3
	1378 (GO)
	1
	1,378
	40 hrs.;
$ 2,540.80
	55,120 hrs.;
$ 3,501,222
	$2,540.80

	
	1016 (GOP)
	1
	1,016
	50 hrs.;
$ 3,176.00
	50,800 hrs.;
$ 3,226,816
	$3,176.00

	Total EOP-012-3
	
	
	2,394
	
	105,920 hrs.;
$ 6,728,038
	



13. ESTIMATE OF THE TOTAL ANNUAL COST BURDEN TO RESPONDENTS

There are no start-up or other non-labor costs.

Total Capital and Start-up cost: $0
Total Operation, Maintenance, and Purchase of Services: $0

All of the costs in the final rule are associated with burden hours (labor) and described in Questions #12 and #15 in this supporting statement.

14. ESTIMATED ANNUALIZED COST TO FEDERAL GOVERNMENT

The Regional Entities and NERC do most of the data processing, monitoring and compliance work for Reliability Standards. Any involvement by the Commission is covered under the FERC-725 (OMB Control No. 1902-0255).  

The Commission does incur the costs associated with obtaining OMB clearance for the two collections under the Paperwork Reduction Act (PRA).  The PRA Administrative Cost is a Federal Cost associated with preparing, issuing, and submitting materials necessary to comply with the Paperwork Reduction Act (PRA) for rulemakings, orders, or any other vehicle used to create, modify, extend, or discontinue an information collection. FERC estimates the annual cost for this effort to be $8,404.00 for each of these collections.  

	FERC-725S
	Number of Employees (FTEs)
	Estimated Annual Federal Cost

	Analysis and Processing of filings
	0
	$0

	Paperwork Reduction Act Administrative Cost[footnoteRef:9] [9:  The PRA Administrative Cost is a Federal Cost associated with preparing, issuing, and submitting materials necessary to comply with the Paperwork Reduction Act (PRA) for rulemakings, orders, or any other vehicle used to create, modify, extend, or discontinue an information collection.] 

	
	$8,404

	TOTAL
	
	$8,404




15. REASONS FOR CHANGES IN BURDEN INCLUDING THE NEED FOR ANY INCREASE

The following table details Reliability Standards EOP-010-1, EOP-011-1, EOP-004-4, EOP-005-3, EOP-006-3, and EOP-008-2 in FERC-725S (OMB Control No. 1902-0270). The burden being added for FERC-725S reflects an increase in total burden hours due to normal fluctuations in industry and better accuracy (separating the standards on the IC list to reflect the accuracy of the reliability standards within 725S. Also, the removal of one-time burden from EOP-011-4 from RD24-1.
	FERC-725S
	Total Request
	Previously Approved
	Change due to Adjustment in Estimate
	Change Due to Agency Discretion

	Annual Number of Responses
	7,344
	2,423
	4,921
	
0


	Annual Time Burden
	198,936
	94,818
	104,118
	0

	Annual Cost Burden ($)
	$0
	$0
	$0
	$0



16. TIME SCHEDULE FOR THE PUBLICATION OF DATA 

There is no publication of data associated with FERC-725S collections of information. 

17. DISPLAY OF THE EXPIRATION DATE 

The expiration dates are posted on ferc.gov at http://www.ferc.gov/docs-filing/info-collections.asp  

18.EXCEPTIONS TO THE CERTIFICATION STATEMENT 

There are no exceptions for FERC-725S. 


